Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
src Directory Reference

## Files
file | brd_driver_hw_03.c
| Board driver for "Sonochan mkII" HW version 03.
file | brd_driver_hw_03.h [code]
| Board driver for "Sonochan mkII" HW version 03.
file | composite_widget.c
| Main file of the USB HID example.
file | composite_widget.h [code]
| Header file of the USB HID example.
file | cs2200.c
| Driver for fractional PLL CS2200.
file | cs2200.h [code]
| Driver for fractional PLL CS2200.
file | cs2200_HAL_AVR32_UC3A3_HW_interface.c
| Hardware Abstraction Layer for PLL CS2200 running on AVR32 UC3A3 architecture.
file | cs2200_HAL_AVR32_UC3A3_HW_interface.h [code]
| Hardware Abstraction Layer for PLL CS2200 running on AVR32 UC3A3 architecture.
file | device_audio_task.c
file | device_audio_task.h [code]
| Management of the USB device mouse Audio task.
file | device_generic_hid.c
| Management of the USB device mouse HID task.
file | device_generic_hid.h [code]
| Management of the USB device mouse HID task.
file | generic_driver.c
| Generic driver.
file | generic_driver.h [code]
| Generic driver.
file | host_audio_task.c
| Management of the USB host mouse HID task.
file | host_audio_task.h [code]
| Management of the USB host mouse HID task.
file | HW.c
| HW controller for generic driver.
file | HW.h [code]
| HW controller for generic driver.
file | HW_bridge_uniprot.c
| Virtual bridge, that connect HW library and universal protocol library.
file | HW_bridge_uniprot.h [code]
| Virtual bridge, that connect HW library and universal protocol library.
file | image.c
file | image.h [code]
file | LCD_5110.c
| Generic driver for LCD used in nokia 5110.
file | LCD_5110.h [code]
| Generic driver for LCD used in nokia 5110.
file | LCD_5110_HAL_AVR32_UC3A3_HW_interface.c
| Hardware Abstraction Layer for AVR32 and LCD used in nokia 5110 Use hardware SPI module on AVR.
file | LCD_5110_HAL_AVR32_UC3A3_HW_interface.h [code]
| Hardware Abstraction Layer for AVR32 and LCD used in nokia 5110. Use hardware SPI module on AVR.
file | sync_control.c
| Synchronization control.
file | sync_control.h [code]
| Synchronization control.
file | taskAK5394A.c
file | taskAK5394A.h [code]
file | taskEXERCISE.c
file | taskEXERCISE.h [code]
file | tlv320aic33.c
| Driver for codec TLV320AIC33.
file | tlv320aic33.h [code]
| Driver for codec TLV320AIC33.
file | tlv320aic33_HAL_AVR32_UC3A3_HW_interface.c
| Hardware Abstraction Layer for codec TLV320AIC33 running on AVR32 UC3A3 architecture.
file | tlv320aic33_HAL_AVR32_UC3A3_HW_interface.h [code]
| Hardware Abstraction Layer for codec TLV320AIC33 running on AVR32 UC3A3 architecture.
file | uac1_device_audio_task.c
| Management of the USB device Audio task.
file | uac1_device_audio_task.h [code]
| Management of the USB device mouse Audio task.
file | uac1_image.c
file | uac1_taskAK5394A.c
file | uac1_taskAK5394A.h [code]
file | uac1_usb_descriptors.c
file | uac1_usb_descriptors.h [code]
file | uac1_usb_specific_request.c
| Processing of USB device specific enumeration requests.
file | uac1_usb_specific_request.h [code]
file | uac2_device_audio_task.c
| Management of the USB device Audio task.
file | uac2_device_audio_task.h [code]
| Management of the USB device mouse Audio task.
file | uac2_image.c
file | uac2_taskAK5394A.c
file | uac2_taskAK5394A.h [code]
file | uac2_usb_descriptors.c
file | uac2_usb_descriptors.h [code]
file | uac2_usb_specific_request.c
| Processing of USB device specific enumeration requests.
file | uac2_usb_specific_request.h [code]
file | uniprot.c
| Universal protocol driver.
file | uniprot.h [code]
| Universal protocol driver.
file | usb_descriptors.c
| USB identifiers.
file | usb_descriptors.h [code]
| USB identifiers.
file | usb_specific_request.c
| Processing of USB device specific enumeration requests.
file | usb_specific_request.h [code]
| Processing of USB device specific enumeration requests.