Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
S_usb_endpoint_audio_descriptor_2 Struct Reference

Usb Standard AS Isochronous Audio Data Endpoint Descriptors pp 4.10.1.1. More...

`#include <usb_descriptors.h>`

## Data Fields
U8 | bLength
U8 | bDescriptorType
U8 | bEndpointAddress
U8 | bmAttributes
U16 | wMaxPacketSize
U8 | bInterval

## Detailed Description

Usb Standard AS Isochronous Audio Data Endpoint Descriptors pp 4.10.1.1.

USB Class-Specific AS Encoder Descriptor pp 4.9.4 USB Encoder Descriptor pp 4.9.4.1 USB Class-Specific AS Decoder Descriptor pp 4.9.5 USB MPEG Decoder Descriptor pp 4.9.5.1 USB AC-3 Decoder Descriptor pp 4.9.5.2 USB WMA Decoder Descriptor pp 4.9.5.3 USB DTS Decoder Descriptor pp 4.9.5.4

## Field Documentation

U8 S_usb_endpoint_audio_descriptor_2::bDescriptorType

U8 S_usb_endpoint_audio_descriptor_2::bEndpointAddress

U8 S_usb_endpoint_audio_descriptor_2::bInterval

U8 S_usb_endpoint_audio_descriptor_2::bLength

U8 S_usb_endpoint_audio_descriptor_2::bmAttributes

U16 S_usb_endpoint_audio_descriptor_2::wMaxPacketSize

The documentation for this struct was generated from the following file:

- /mnt/data/GENTOO_FILES/home/k1ll3r/Dokumenty/Diplomka/Sonochan_II/FW_sdr_widget/sdr-widget/src/usb_descriptors.h