Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions | Variables
composite_widget.c File Reference

Main file of the USB HID example. More...

`#include <stdio.h>`
`#include "compiler.h"`
`#include "board.h"`
`#include "print_funcs.h"`
`#include "intc.h"`
`#include "pm.h"`
`#include "gpio.h"`
`#include "wdt.h"`
`#include "rtc.h"`
`#include "FreeRTOS.h"`
`#include "image.h"`
`#include "composite_widget.h"`
`#include "brd_driver_hw_03.h"`

## Functions
int | main (void)
| Main function. Execution starts here. More...

## Variables
xSemaphoreHandle | mutexEP_IN
pm_freq_param_t | pm_freq_param

## Detailed Description

Main file of the USB HID example.

- Compiler: IAR EWAVR32 and GNU GCC for AVR32
- Supported devices: All AVR32 devices with a USB module can be used.
- AppNote:

Author
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

## Function Documentation

int main | ( | void | ) |  |

Main function. Execution starts here.

Return values

  42 | Fatal error.

## Variable Documentation

xSemaphoreHandle mutexEP_IN

pm_freq_param_t pm_freq_param

Initial value:
=
{
.cpu_f = FCPU_HZ
, .pba_f = FPBA_HZ
, .osc0_f = FOSC0
, .osc0_startup = OSC0_STARTUP
}