Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
uac2_device_audio_task.h File Reference

Management of the USB device mouse Audio task. More...

`#include "conf_usb.h"`

Go to the source code of this file.

## Functions
void | uac2_device_audio_task_init (U8 ep_in, U8 ep_out, U8 ep_out_fb)
| This function initializes the hardware/software resources required for device Audio task. More...
void | uac2_device_audio_task (void)

## Detailed Description

Management of the USB device mouse Audio task.

This file manages the USB device mouse Audio task.

- Compiler: IAR EWAVR32 and GNU GCC for AVR32
- Supported devices: All AVR32 devices with a USB module can be used.
- AppNote:

Author
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

## Function Documentation

void uac2_device_audio_task | ( | void | ) |  |

void uac2_device_audio_task_init | ( | U8 | ep_in,
|  | U8 | ep_out,
|  | U8 | ep_out_fb
| ) |  |

This function initializes the hardware/software resources required for device Audio task.