Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w
- x

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - d -

- dac_dual_rate_mode_is_disabled : tlv320aic33.h
- dac_dual_rate_mode_is_enabled : tlv320aic33.h
- data_to_transfer : uac2_usb_specific_request.c , usb_specific_request.c , uac1_usb_specific_request.c
- DEVICE0 : HW.h
- DEVICE1 : HW.h
- DEVICE2 : HW.h
- device_Cfg_1_t : cs2200.h
- DEVICE_CLASS : usb_descriptors.h
- device_ctrl_t : cs2200.h
- device_generic_HID_init() : device_generic_hid.c , device_generic_hid.h
- DEVICE_GENERIC_HID_SUPPORT_UNIPROT : device_generic_hid.h
- device_generic_hid_task() : device_generic_hid.h , device_generic_hid.c
- DEVICE_GENERIC_HID_UNIPROT_PIPE : device_generic_hid.h
- device_id_t : cs2200.h
- DEVICE_PROTOCOL : usb_descriptors.h
- DEVICE_STATUS : usb_descriptors.h
- DEVICE_SUB_CLASS : usb_descriptors.h
- dg8saqBuffer : usb_specific_request.c
- digital_mic_support_disabled : tlv320aic33.h
- digital_mic_support_enabled_oversampling_128 : tlv320aic33.h
- digital_mic_support_enabled_oversampling_32 : tlv320aic33.h
- digital_mic_support_enabled_oversampling_64 : tlv320aic33.h
- disable_3D_digital_effect : tlv320aic33.h
- do_not_3state_DOUT_when_valid_data_is_not_being_send : tlv320aic33.h
- driver_power_on_time_0us : tlv320aic33.h
- driver_power_on_time_100ms : tlv320aic33.h
- driver_power_on_time_100us : tlv320aic33.h
- driver_power_on_time_10ms : tlv320aic33.h
- driver_power_on_time_10us : tlv320aic33.h
- driver_power_on_time_1ms : tlv320aic33.h
- driver_power_on_time_200ms : tlv320aic33.h
- driver_power_on_time_2s : tlv320aic33.h
- driver_power_on_time_400ms : tlv320aic33.h
- driver_power_on_time_4s : tlv320aic33.h
- driver_power_on_time_50ms : tlv320aic33.h
- driver_power_on_time_800ms : tlv320aic33.h
- driver_ramp_up_step_time_0ms : tlv320aic33.h
- driver_ramp_up_step_time_1ms : tlv320aic33.h
- driver_ramp_up_step_time_2ms : tlv320aic33.h
- driver_ramp_up_step_time_4ms : tlv320aic33.h
- DSC_INTERFACE_AS : uac2_usb_descriptors.h
- DSC_INTERFACE_AS_OUT : uac2_usb_descriptors.h
- DSC_INTERFACE_AUDIO : uac2_usb_descriptors.h , uac1_usb_descriptors.h
- DSC_INTERFACE_DG8SAQ : uac2_usb_descriptors.h
- DSC_INTERFACE_HID : uac1_usb_descriptors.h