Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Variables
device_audio_task.h File Reference

Management of the USB device mouse Audio task. More...

`#include "conf_usb.h"`

Go to the source code of this file.

## Variables
volatile Bool | mute
volatile Bool | spk_mute
volatile U32 | FB_rate
S16 | volume
S16 | spk_volume

## Detailed Description

Management of the USB device mouse Audio task.

This file manages the USB device mouse Audio task.

- Compiler: IAR EWAVR32 and GNU GCC for AVR32
- Supported devices: All AVR32 devices with a USB module can be used.
- AppNote:

Author
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

## Variable Documentation

volatile U32 FB_rate

volatile Bool mute

Public : (bit) mute mute is set to TRUE when ACTIVE mute is set to FALSE otherwise /

volatile Bool spk_mute

S16 spk_volume

S16 volume