Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages

### - b -

- BDR_DRV_ADC_ADDRESS : brd_driver_hw_03.h
- BELONGS_AUDIO_INTERFACE_IN : uac1_usb_descriptors.h
- BELONGS_AUDIO_INTERFACE_OUT : uac1_usb_descriptors.h
- BRD_DRV_ADC_CLK_SOURCE : brd_driver_hw_03.h
- BRD_DRV_ADC_CON_VOLTAGE_CHANNEL : brd_driver_hw_03.h
- BRD_DRV_ADC_CON_VOLTAGE_FUNCTION : brd_driver_hw_03.h
- BRD_DRV_ADC_CON_VOLTAGE_PIN : brd_driver_hw_03.h
- BRD_DRV_ADC_DATA : brd_driver_hw_03.h
- BRD_DRV_ADC_DATA_simple : brd_driver_hw_03.h
- BRD_DRV_ADC_HIGH_VOL_MIN : brd_driver_hw_03.c
- BRD_DRV_ADC_PRESCAL : brd_driver_hw_03.h
- BRD_DRV_ADC_PRESCALLED_CLK : brd_driver_hw_03.h
- BRD_DRV_ADC_SAMPLE_HOLD_TIME : brd_driver_hw_03.h
- BRD_DRV_ADC_SAVE_VOL_MIN : brd_driver_hw_03.c
- BRD_DRV_ADC_START_UP_TIME : brd_driver_hw_03.h
- BRD_DRV_ADC_UPDATE_THRESHOLD : brd_driver_hw_03.h
- BRD_DRV_ADC_VOLUME_CONTROL_CHANNEL : brd_driver_hw_03.h
- BRD_DRV_ADC_VOLUME_CONTROL_FUNCTION : brd_driver_hw_03.h
- BRD_DRV_ADC_VOLUME_CONTROL_PIN : brd_driver_hw_03.h
- BRD_DRV_BCLK_EN_A_PIN : brd_driver_hw_03.h
- BRD_DRV_BCLK_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_BUTTON_REFRESH_PERIOD : brd_driver_hw_03.h
- BRD_DRV_CON_NOT_POWERED : brd_driver_hw_03.h
- BRD_DRV_CON_VOL_HIGH : brd_driver_hw_03.h
- BRD_DRV_CON_VOL_LOW : brd_driver_hw_03.h
- BRD_DRV_CON_VOL_SAVE : brd_driver_hw_03.h
- BRD_DRV_DEFAULT_HEADPHONES_VOLUME_IN_DB : brd_driver_hw_03.h
- BRD_DRV_EN_ADC_CHANNEL : brd_driver_hw_03.h
- BRD_DRV_EN_ADC_CHANNEL_simple : brd_driver_hw_03.h
- BRD_DRV_ERROR_SIG_PIN : brd_driver_hw_03.h
- BRD_DRV_FS_EN_A_PIN : brd_driver_hw_03.h
- BRD_DRV_FS_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_IO_AS_INPUT : brd_driver_hw_03.h
- BRD_DRV_IO_AS_INPUT_simple : brd_driver_hw_03.h
- BRD_DRV_IO_HIGH : brd_driver_hw_03.h
- BRD_DRV_IO_HIGH_simple : brd_driver_hw_03.h
- BRD_DRV_IO_LOW : brd_driver_hw_03.h
- BRD_DRV_IO_LOW_simple : brd_driver_hw_03.h
- BRD_DRV_IO_READ : brd_driver_hw_03.h
- BRD_DRV_IO_READ_simple : brd_driver_hw_03.h
- BRD_DRV_IS_ADC_DONE : brd_driver_hw_03.h
- BRD_DRV_IS_ADC_DONE_simple : brd_driver_hw_03.h
- BRD_DRV_LCD_HP_VOLUME_LINE : brd_driver_hw_03.h
- BRD_DRV_LCD_INFO_MSG_LINE : brd_driver_hw_03.h
- BRD_DRV_LCD_LOGO_LINE : brd_driver_hw_03.h
- BRD_DRV_LCD_WARN_MSG_LINE : brd_driver_hw_03.h
- BRD_DRV_LCD_WRITE_FAIL : brd_driver_hw_03.h
- BRD_DRV_LOCK_ADC_MODULE_IF_RTOS : brd_driver_hw_03.h
- BRD_DRV_MAX_CMD_ID : brd_driver_hw_03.c
- BRD_DRV_MCLK_EN_A_PIN : brd_driver_hw_03.h
- BRD_DRV_MCLK_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_MSG_ADC_INIT_FAIL : brd_driver_hw_03.h
- BRD_DRV_MSG_CODEC_INIT_FAIL : brd_driver_hw_03.h
- BRD_DRV_MSG_DRAW_LOGO_FAIL : brd_driver_hw_03.h
- BRD_DRV_MSG_ERR_MSG_CLEARED : brd_driver_hw_03.h
- BRD_DRV_MSG_ERROR_CLEANED : brd_driver_hw_03.h
- BRD_DRV_MSG_LCD_INIT_FAIL : brd_driver_hw_03.h
- BRD_DRV_MSG_MUTE_BTN_PRESSED : brd_driver_hw_03.h
- BRD_DRV_MSG_MUTE_BTN_RELEASED : brd_driver_hw_03.h
- BRD_DRV_MSG_MUTE_FALLING_EDGE : brd_driver_hw_03.h
- BRD_DRV_MSG_MUTE_RISING_EDGE : brd_driver_hw_03.h
- BRD_DRV_MSG_PLL_SET_SAVE_FLAG_FAIL : brd_driver_hw_03.h
- BRD_DRV_MSG_RESET_I2S_DONE : brd_driver_hw_03.h
- BRD_DRV_MSG_RESET_I2S_INPUT_OFF : brd_driver_hw_03.h
- BRD_DRV_MSG_RESET_I2S_INPUT_ON : brd_driver_hw_03.h
- BRD_DRV_MSG_RESET_I2S_SET_TO_HIGH : brd_driver_hw_03.h
- BRD_DRV_MSG_RESET_I2S_SET_TO_LOW : brd_driver_hw_03.h
- BRD_DRV_MSG_RST_I2S_BTN_PRESSED : brd_driver_hw_03.h
- BRD_DRV_MSG_RST_I2S_BTN_RELEASED : brd_driver_hw_03.h
- BRD_DRV_MSG_RST_I2S_FALLING_EDGE : brd_driver_hw_03.h
- BRD_DRV_MSG_RST_I2S_RISING_EDGE : brd_driver_hw_03.h
- BRD_DRV_MSG_SONOCHAN_MK_II : brd_driver_hw_03.h
- BRD_DRV_MUTE_BTN_PIN : brd_driver_hw_03.h
- BRD_DRV_MUTE_EN_A_PIN : brd_driver_hw_03.h
- BRD_DRV_MUTE_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_MUTE_IN_MUTE_OFF : brd_driver_hw_03.h
- BRD_DRV_MUTE_IN_MUTE_ON : brd_driver_hw_03.h
- BRD_DRV_MUTE_OUT_MUTE_OFF : brd_driver_hw_03.h
- BRD_DRV_MUTE_OUT_MUTE_ON : brd_driver_hw_03.h
- BRD_DRV_MUTE_PIN : brd_driver_hw_03.h
- BRD_DRV_RESET_I2S_BTN_PIN : brd_driver_hw_03.h
- BRD_DRV_RESET_I2S_PERIOD : brd_driver_hw_03.h
- BRD_DRV_RESET_I2S_PIN : brd_driver_hw_03.h
- BRD_DRV_RST_EN_A_PIN : brd_driver_hw_03.h
- BRD_DRV_RST_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_RTOS_CREATE_MUTEX : brd_driver_hw_03.h
- BRD_DRV_RX_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_SHORT_PRESS : brd_driver_hw_03.h
- BRD_DRV_SUPPORT_GENERIC_DRIVER : brd_driver_hw_03.h
- BRD_DRV_SUPPORT_RTOS : brd_driver_hw_03.h
- BRD_DRV_TLV_FAILED_SET_HEADPHONE_VOL_DB : brd_driver_hw_03.h
- BRD_DRV_TX_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_UNLOCK_ADC_MODULE_IF_RTOS : brd_driver_hw_03.h