Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
uac2_taskAK5394A.c File Reference
`#include "usart.h"`
`#include "conf_usb.h"`
`#include <avr32/io.h>`
`#include "board.h"`
`#include "usb_drv.h"`
`#include "gpio.h"`
`#include "ssc_i2s.h"`
`#include "pm.h"`
`#include "pdca.h"`
`#include "usb_standard_request.h"`
`#include "usb_specific_request.h"`
`#include "device_audio_task.h"`
`#include "uac2_device_audio_task.h"`
`#include "taskAK5394A.h"`
`#include "uac2_taskAK5394A.h"`

## Functions
void | uac2_AK5394A_task (void *pvParameters)
| Entry point of the AK5394A task management. More...
void | uac2_AK5394A_task_init (void)
| This function initializes the hardware/software resources required for device CDC task. More...

## Function Documentation

void uac2_AK5394A_task | ( | void * | pvParameters) |  |

Entry point of the AK5394A task management.

void uac2_AK5394A_task_init | ( | void | ) |  |

This function initializes the hardware/software resources required for device CDC task.