Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Variables
composite_widget.h File Reference

Header file of the USB HID example. More...

`#include "FreeRTOS.h"`
`#include "task.h"`
`#include "queue.h"`
`#include "semphr.h"`

Go to the source code of this file.

## Macros
#define | COUNTER_TIME_OUT 1000000L
#define | RTC_COUNTER_MAX 1150000

## Variables
xSemaphoreHandle | mutexEP_IN

## Detailed Description

Header file of the USB HID example.

- Compiler: IAR EWAVR32 and GNU GCC for AVR32
- Supported devices: All AVR32 devices with a USB module can be used.
- AppNote:

Author
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

## Macro Definition Documentation

#define COUNTER_TIME_OUT 1000000L

#define RTC_COUNTER_MAX 1150000

## Variable Documentation

xSemaphoreHandle mutexEP_IN