Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w
- x

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - g -

- g_cs_feature : host_audio_task.c
- g_cs_num_features_unit : host_audio_task.c
- g_n_bits_per_sample : host_audio_task.c
- g_n_channels : host_audio_task.c
- g_sample_freq : host_audio_task.c
- g_u8_report_rate : usb_specific_request.c , usb_specific_request.h
- gapLimit0 : uac2_device_audio_task.c
- gapLimit1 : uac2_device_audio_task.c
- GD_CMD_ID_NOT_EQUAL_IN_FLASH : generic_driver.h
- GD_DATA_TYPE : generic_driver.h
- GD_FAIL : generic_driver.h
- gd_get_setting() : generic_driver.c , generic_driver.h
- gd_if_big_endian_convert_big_to_little_endian() : generic_driver.c
- gd_if_big_endian_convert_little_to_big_endian() : generic_driver.c
- GD_INCORRECT_CMD_ID : generic_driver.h
- GD_INCORRECT_DEVICE_ID : generic_driver.h
- GD_INCORRECT_PARAMETER : generic_driver.h
- GD_MAX_STRING_SIZE : generic_driver.h
- GD_POINTER_TO_FUNCTION : generic_driver.h
- gd_read_byte_ro_mem : generic_driver.h
- gd_read_dword_ro_mem : generic_driver.h
- gd_read_word_ro_mem : generic_driver.h
- GD_RES_CODE : generic_driver.h
- GD_RES_CODE_DEFINED : generic_driver.h
- gd_set_setting() : generic_driver.h , generic_driver.c
- GD_SUCCESS : generic_driver.h
- gd_void_function() : generic_driver.h , generic_driver.c
- gd_void_value : generic_driver.c , generic_driver.h
- GET_ENCAPSULATED_RESPONSE : usb_specific_request.h
- GET_LINE_CODING : usb_specific_request.h
- global_Cfg_t : cs2200.h
- group_type : generic_driver.h