Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w
- x

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - b -

- BDR_DRV_ADC_ADDRESS : brd_driver_hw_03.h
- BELONGS_AUDIO_INTERFACE_IN : uac1_usb_descriptors.h
- BELONGS_AUDIO_INTERFACE_OUT : uac1_usb_descriptors.h
- bit_clk_and_word_clk_not_transmitt_in_master_mode_if_power_dwn : tlv320aic33.h
- bit_clk_and_word_clk_transmitt_in_master_mode_if_power_dwn : tlv320aic33.h
- bit_clock_is_an_input : tlv320aic33.h
- bit_clock_is_an_output : tlv320aic33.h
- BRD_DRV_ADC_CLK_SOURCE : brd_driver_hw_03.h
- BRD_DRV_ADC_CON_VOLTAGE_CHANNEL : brd_driver_hw_03.h
- BRD_DRV_ADC_CON_VOLTAGE_FUNCTION : brd_driver_hw_03.h
- BRD_DRV_ADC_CON_VOLTAGE_PIN : brd_driver_hw_03.h
- BRD_DRV_ADC_DATA : brd_driver_hw_03.h
- BRD_DRV_ADC_DATA_simple : brd_driver_hw_03.h
- BRD_DRV_ADC_HIGH_VOL_MIN : brd_driver_hw_03.c
- brd_drv_adc_init() : brd_driver_hw_03.c
- BRD_DRV_ADC_PRESCAL : brd_driver_hw_03.h
- BRD_DRV_ADC_PRESCALLED_CLK : brd_driver_hw_03.h
- BRD_DRV_ADC_SAMPLE_HOLD_TIME : brd_driver_hw_03.h
- BRD_DRV_ADC_SAVE_VOL_MIN : brd_driver_hw_03.c
- BRD_DRV_ADC_START_UP_TIME : brd_driver_hw_03.h
- BRD_DRV_ADC_UPDATE_THRESHOLD : brd_driver_hw_03.h
- BRD_DRV_ADC_VOLUME_CONTROL_CHANNEL : brd_driver_hw_03.h
- BRD_DRV_ADC_VOLUME_CONTROL_FUNCTION : brd_driver_hw_03.h
- BRD_DRV_ADC_VOLUME_CONTROL_PIN : brd_driver_hw_03.h
- BRD_DRV_BCLK_EN_A_PIN : brd_driver_hw_03.h
- BRD_DRV_BCLK_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_BUTTON_REFRESH_PERIOD : brd_driver_hw_03.h
- brd_drv_con_high_vol : brd_driver_hw_03.h
- brd_drv_con_low_vol : brd_driver_hw_03.h
- BRD_DRV_CON_NOT_POWERED : brd_driver_hw_03.h
- brd_drv_con_save_vol : brd_driver_hw_03.h
- brd_drv_con_undefined : brd_driver_hw_03.h
- BRD_DRV_CON_VOL_HIGH : brd_driver_hw_03.h
- BRD_DRV_CON_VOL_LOW : brd_driver_hw_03.h
- BRD_DRV_CON_VOL_SAVE : brd_driver_hw_03.h
- BRD_DRV_config_table : brd_driver_hw_03.c
- BRD_DRV_config_table_flash : brd_driver_hw_03.h
- BRD_DRV_DEFAULT_HEADPHONES_VOLUME_IN_DB : brd_driver_hw_03.h
- brd_drv_dir_hiz : brd_driver_hw_03.h
- brd_drv_dir_in : brd_driver_hw_03.h
- brd_drv_dir_out : brd_driver_hw_03.h
- brd_drv_draw_logo() : brd_driver_hw_03.c , brd_driver_hw_03.h
- BRD_DRV_EN_ADC_CHANNEL : brd_driver_hw_03.h
- BRD_DRV_EN_ADC_CHANNEL_simple : brd_driver_hw_03.h
- BRD_DRV_ERROR_SIG_PIN : brd_driver_hw_03.h
- BRD_DRV_FS_EN_A_PIN : brd_driver_hw_03.h
- BRD_DRV_FS_EN_B_PIN : brd_driver_hw_03.h
- brd_drv_init() : brd_driver_hw_03.c , brd_driver_hw_03.h
- BRD_DRV_IO_AS_INPUT : brd_driver_hw_03.h
- BRD_DRV_IO_AS_INPUT_simple : brd_driver_hw_03.h
- BRD_DRV_IO_HIGH : brd_driver_hw_03.h
- BRD_DRV_IO_HIGH_simple : brd_driver_hw_03.h
- BRD_DRV_IO_LOW : brd_driver_hw_03.h
- BRD_DRV_IO_LOW_simple : brd_driver_hw_03.h
- BRD_DRV_IO_READ : brd_driver_hw_03.h
- BRD_DRV_IO_READ_simple : brd_driver_hw_03.h
- BRD_DRV_IS_ADC_DONE : brd_driver_hw_03.h
- BRD_DRV_IS_ADC_DONE_simple : brd_driver_hw_03.h
- BRD_DRV_LCD_HP_VOLUME_LINE : brd_driver_hw_03.h
- BRD_DRV_LCD_INFO_MSG_LINE : brd_driver_hw_03.h
- BRD_DRV_LCD_LOGO_LINE : brd_driver_hw_03.h
- BRD_DRV_LCD_WARN_MSG_LINE : brd_driver_hw_03.h
- BRD_DRV_LCD_WRITE_FAIL : brd_driver_hw_03.h
- BRD_DRV_LOCK_ADC_MODULE_IF_RTOS : brd_driver_hw_03.h
- BRD_DRV_MAX_CMD_ID : brd_driver_hw_03.c
- BRD_DRV_MCLK_EN_A_PIN : brd_driver_hw_03.h
- BRD_DRV_MCLK_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_metadata : brd_driver_hw_03.c , brd_driver_hw_03.h
- BRD_DRV_MSG_ADC_INIT_FAIL : brd_driver_hw_03.h
- BRD_DRV_MSG_CODEC_INIT_FAIL : brd_driver_hw_03.h
- BRD_DRV_MSG_DRAW_LOGO_FAIL : brd_driver_hw_03.h
- BRD_DRV_MSG_ERR_MSG_CLEARED : brd_driver_hw_03.h
- BRD_DRV_MSG_ERROR_CLEANED : brd_driver_hw_03.h
- BRD_DRV_MSG_LCD_INIT_FAIL : brd_driver_hw_03.h
- BRD_DRV_MSG_MUTE_BTN_PRESSED : brd_driver_hw_03.h
- BRD_DRV_MSG_MUTE_BTN_RELEASED : brd_driver_hw_03.h
- BRD_DRV_MSG_MUTE_FALLING_EDGE : brd_driver_hw_03.h
- BRD_DRV_MSG_MUTE_RISING_EDGE : brd_driver_hw_03.h
- BRD_DRV_MSG_PLL_SET_SAVE_FLAG_FAIL : brd_driver_hw_03.h
- BRD_DRV_MSG_RESET_I2S_DONE : brd_driver_hw_03.h
- BRD_DRV_MSG_RESET_I2S_INPUT_OFF : brd_driver_hw_03.h
- BRD_DRV_MSG_RESET_I2S_INPUT_ON : brd_driver_hw_03.h
- BRD_DRV_MSG_RESET_I2S_SET_TO_HIGH : brd_driver_hw_03.h
- BRD_DRV_MSG_RESET_I2S_SET_TO_LOW : brd_driver_hw_03.h
- BRD_DRV_MSG_RST_I2S_BTN_PRESSED : brd_driver_hw_03.h
- BRD_DRV_MSG_RST_I2S_BTN_RELEASED : brd_driver_hw_03.h
- BRD_DRV_MSG_RST_I2S_FALLING_EDGE : brd_driver_hw_03.h
- BRD_DRV_MSG_RST_I2S_RISING_EDGE : brd_driver_hw_03.h
- BRD_DRV_MSG_SONOCHAN_MK_II : brd_driver_hw_03.h
- BRD_DRV_MUTE_BTN_PIN : brd_driver_hw_03.h
- BRD_DRV_MUTE_EN_A_PIN : brd_driver_hw_03.h
- BRD_DRV_MUTE_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_MUTE_IN_MUTE_OFF : brd_driver_hw_03.h
- BRD_DRV_MUTE_IN_MUTE_ON : brd_driver_hw_03.h
- BRD_DRV_MUTE_OUT_MUTE_OFF : brd_driver_hw_03.h
- BRD_DRV_MUTE_OUT_MUTE_ON : brd_driver_hw_03.h
- BRD_DRV_MUTE_PIN : brd_driver_hw_03.h
- brd_drv_pre_init() : brd_driver_hw_03.c , brd_driver_hw_03.h
- brd_drv_process_mute_button() : brd_driver_hw_03.c
- brd_drv_process_mute_signal() : brd_driver_hw_03.c
- brd_drv_process_rst_i2s_button() : brd_driver_hw_03.c
- brd_drv_process_rst_i2s_signal() : brd_driver_hw_03.c
- brd_drv_reset_i2s() : brd_driver_hw_03.h , brd_driver_hw_03.c
- BRD_DRV_RESET_I2S_BTN_PIN : brd_driver_hw_03.h
- BRD_DRV_RESET_I2S_PERIOD : brd_driver_hw_03.h
- BRD_DRV_RESET_I2S_PIN : brd_driver_hw_03.h
- BRD_DRV_RST_EN_A_PIN : brd_driver_hw_03.h
- BRD_DRV_RST_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_RTOS_CREATE_MUTEX : brd_driver_hw_03.h
- BRD_DRV_RX_EN_B_PIN : brd_driver_hw_03.h
- brd_drv_send_error_msg() : brd_driver_hw_03.h , brd_driver_hw_03.c
- brd_drv_send_msg() : brd_driver_hw_03.h , brd_driver_hw_03.c
- brd_drv_send_warning_msg() : brd_driver_hw_03.h , brd_driver_hw_03.c
- brd_drv_set_bclk_dir() : brd_driver_hw_03.h , brd_driver_hw_03.c
- brd_drv_set_frame_sync_dir() : brd_driver_hw_03.h , brd_driver_hw_03.c
- brd_drv_set_isolators_to_HiZ() : brd_driver_hw_03.c , brd_driver_hw_03.h
- brd_drv_set_mclk_dir() : brd_driver_hw_03.c , brd_driver_hw_03.h
- brd_drv_set_mute() : brd_driver_hw_03.h , brd_driver_hw_03.c
- brd_drv_set_mute_dir() : brd_driver_hw_03.c , brd_driver_hw_03.h
- brd_drv_set_rst_i2s() : brd_driver_hw_03.h , brd_driver_hw_03.c
- brd_drv_set_rst_i2s_dir() : brd_driver_hw_03.c , brd_driver_hw_03.h
- brd_drv_set_rx_data_dir() : brd_driver_hw_03.h , brd_driver_hw_03.c
- brd_drv_set_tx_data_dir() : brd_driver_hw_03.c , brd_driver_hw_03.h
- BRD_DRV_SHORT_PRESS : brd_driver_hw_03.h
- brd_drv_show_volume() : brd_driver_hw_03.c , brd_driver_hw_03.h
- BRD_DRV_SUPPORT_GENERIC_DRIVER : brd_driver_hw_03.h
- BRD_DRV_SUPPORT_RTOS : brd_driver_hw_03.h
- brd_drv_task() : brd_driver_hw_03.c , brd_driver_hw_03.h
- brd_drv_task_FreeRTOS() : brd_driver_hw_03.c
- brd_drv_TLV_default() : brd_driver_hw_03.c
- BRD_DRV_TLV_FAILED_SET_HEADPHONE_VOL_DB : brd_driver_hw_03.h
- BRD_DRV_TX_EN_B_PIN : brd_driver_hw_03.h
- BRD_DRV_UNLOCK_ADC_MODULE_IF_RTOS : brd_driver_hw_03.h
- bridge_init() : HW_bridge_uniprot.c , HW_bridge_uniprot.h
- BRIDGE_STATE : HW_bridge_uniprot.h
- bridge_task() : HW_bridge_uniprot.c , HW_bridge_uniprot.h
- bridge_task_FreeRTOS() : HW_bridge_uniprot.h , HW_bridge_uniprot.c
- byte_count : host_audio_task.c