# ==<| Sonochan mkII |>==

## Description:
 * Polymorph usb soundcard (USB <--> I2S) based on AVR32 UC3A3256
 * As clock source generator is used CS2200
 * On board is DAC TLV320AIC33 which can sniff I2S bus (RX or TX data)
 * Supported sampling frequencies: 8000, 11025, 16000, 22050, 24000, 32000,
   44100 and 48000 Hz
 * Bit precision: 24 bit
 * Control thru USB HID (HW bridge uniprot)
 * Using SDR Widget core

## Get source code!
 `git clone https://MartinStejskal@bitbucket.org/MartinStejskal/sonochan-ii_widget.git`

