Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- w

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages

### - m -

- MaxPower : S_usb_configuration_descriptor
- MIC3LInputLevelControlForLeftADCPGAMix : p0_r17_MIC3L_R_To_Left_ADC_Control_t
- MIC3LInputLevelControlForRightADCPGAMix : p0_r18_MIC3L_R_To_Right_ADC_Control_t
- MIC3RInputLevelControlForLeftADCPGAMix : p0_r17_MIC3L_R_To_Left_ADC_Control_t
- MIC3RInputLevelControlForRightADCPGAMix : p0_r18_MIC3L_R_To_Right_ADC_Control_t
- mic_as_alt0 : S_usb_user_configuration_descriptor , S_usb_user_configuration_descriptor_one_freq
- mic_as_alt1 : S_usb_user_configuration_descriptor , S_usb_user_configuration_descriptor_one_freq
- mic_fea_unit : S_usb_user_configuration_descriptor , S_usb_user_configuration_descriptor_one_freq , S_usb_user_configuration_descriptor
- mic_format_type : S_usb_user_configuration_descriptor , S_usb_user_configuration_descriptor_one_freq
- mic_g_as : S_usb_user_configuration_descriptor , S_usb_user_configuration_descriptor_one_freq , S_usb_user_configuration_descriptor
- mic_in_ter : S_usb_user_configuration_descriptor_one_freq , S_usb_user_configuration_descriptor
- mic_out_ter : S_usb_user_configuration_descriptor_one_freq , S_usb_user_configuration_descriptor
- MICBIASLevelControl : p0_r25_MICBIAS_Control_t