Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Todo List

Group Basic settings for TWI
  Try to remove this dependency
Group Basic settings for TWI
  Try to remove this dependency
Group Basic settings SPI interface
  Try remove this dependency
Global BRD_DRV_config_table_flash []

  Move definitions here

  Try to remove this dependency

Global brd_drv_reset_i2s (void)
  Complete this function. it need functions to set I/O for isolators
Global cdc_set_control_line_state (void)
  Manages here hardware flow control...
Global TLV320AIC33_TWI_ADDRESS
  Complete doc
Global TLV320AIC33_TWI_BAUDRATE
  Check device address (1 of 4)
Global uac1_device_audio_task (void *pvParameters)
  [Martin] It that code really needed? It looks like that num_samples is changed only by 1. Try and add more conditions -> set more proper num_samples
Global x_image_task_init (void)
  More process