Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- n
- p
- r
- s
- t
- u
- v
- w

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages

### - a -

- adc_dual_rate_mode_is_disabled : tlv320aic33.h
- adc_dual_rate_mode_is_enabled : tlv320aic33.h
- all_programmed_gains_to_HPLOUT_have_been_applied_yet : tlv320aic33.h
- all_programmed_gains_to_HPROUT_have_been_applied_yet : tlv320aic33.h
- audio_data_word_length_16bit : tlv320aic33.h
- audio_data_word_length_20bit : tlv320aic33.h
- audio_data_word_length_24bit : tlv320aic33.h
- audio_data_word_length_32bit : tlv320aic33.h

### - b -

- bit_clk_and_word_clk_not_transmitt_in_master_mode_if_power_dwn : tlv320aic33.h
- bit_clk_and_word_clk_transmitt_in_master_mode_if_power_dwn : tlv320aic33.h
- bit_clock_is_an_input : tlv320aic33.h
- bit_clock_is_an_output : tlv320aic33.h
- brd_drv_con_high_vol : brd_driver_hw_03.h
- brd_drv_con_low_vol : brd_driver_hw_03.h
- brd_drv_con_save_vol : brd_driver_hw_03.h
- brd_drv_con_undefined : brd_driver_hw_03.h
- brd_drv_dir_hiz : brd_driver_hw_03.h
- brd_drv_dir_in : brd_driver_hw_03.h
- brd_drv_dir_out : brd_driver_hw_03.h

### - c -

- char_type : generic_driver.h
- CLKDIV_IN_uses_BCLK : tlv320aic33.h
- CLKDIV_IN_uses_GPIO2 : tlv320aic33.h
- CLKDIV_IN_uses_MCLK : tlv320aic33.h
- clock_256_transfer_mode : tlv320aic33.h
- common_output_voltage_generated_from_bandgap_reference : tlv320aic33.h
- common_output_voltage_generated_from_resistor_divider : tlv320aic33.h
- continuous_transfer_mode : tlv320aic33.h
- CS2200_ERROR : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_ERROR_TWI_INVALID_PARAMETER : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_ERROR_TWI_NACK : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_ERROR_TWI_TIMEOUT : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_INPUT_DIVIDER_1x : cs2200.h
- CS2200_INPUT_DIVIDER_2x : cs2200.h
- CS2200_INPUT_DIVIDER_4x : cs2200.h
- CS2200_OK : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_R_MOD__DIV_16x : cs2200.h
- CS2200_R_MOD__DIV_2x : cs2200.h
- CS2200_R_MOD__DIV_4x : cs2200.h
- CS2200_R_MOD__DIV_8x : cs2200.h
- CS2200_R_MOD__MUL_1x : cs2200.h
- CS2200_R_MOD__MUL_2x : cs2200.h
- CS2200_R_MOD__MUL_4x : cs2200.h
- CS2200_R_MOD__MUL_8x : cs2200.h

### - d -

- dac_dual_rate_mode_is_disabled : tlv320aic33.h
- dac_dual_rate_mode_is_enabled : tlv320aic33.h
- digital_mic_support_disabled : tlv320aic33.h
- digital_mic_support_enabled_oversampling_128 : tlv320aic33.h
- digital_mic_support_enabled_oversampling_32 : tlv320aic33.h
- digital_mic_support_enabled_oversampling_64 : tlv320aic33.h
- disable_3D_digital_effect : tlv320aic33.h
- do_not_3state_DOUT_when_valid_data_is_not_being_send : tlv320aic33.h
- driver_power_on_time_0us : tlv320aic33.h
- driver_power_on_time_100ms : tlv320aic33.h
- driver_power_on_time_100us : tlv320aic33.h
- driver_power_on_time_10ms : tlv320aic33.h
- driver_power_on_time_10us : tlv320aic33.h
- driver_power_on_time_1ms : tlv320aic33.h
- driver_power_on_time_200ms : tlv320aic33.h
- driver_power_on_time_2s : tlv320aic33.h
- driver_power_on_time_400ms : tlv320aic33.h
- driver_power_on_time_4s : tlv320aic33.h
- driver_power_on_time_50ms : tlv320aic33.h
- driver_power_on_time_800ms : tlv320aic33.h
- driver_ramp_up_step_time_0ms : tlv320aic33.h
- driver_ramp_up_step_time_1ms : tlv320aic33.h
- driver_ramp_up_step_time_2ms : tlv320aic33.h
- driver_ramp_up_step_time_4ms : tlv320aic33.h

### - e -

- enable_3D_digital_effect : tlv320aic33.h

### - f -

- float_type : generic_driver.h
- fsref_44_1khz : tlv320aic33.h
- fsref_48khz : tlv320aic33.h

### - g -

- GD_CMD_ID_NOT_EQUAL_IN_FLASH : generic_driver.h
- GD_FAIL : generic_driver.h
- GD_INCORRECT_CMD_ID : generic_driver.h
- GD_INCORRECT_DEVICE_ID : generic_driver.h
- GD_INCORRECT_PARAMETER : generic_driver.h
- GD_SUCCESS : generic_driver.h
- group_type : generic_driver.h

### - h -

- HPLCOM_is_constant_VCM : tlv320aic33.h
- HPLCOM_is_differential_of_HPLOUT : tlv320aic33.h
- HPLCOM_is_single_ended : tlv320aic33.h
- HPLOUT_is_3_stated_with_pwr_dwn : tlv320aic33.h
- HPLOUT_is_weakly_driven_to_common_mode_when_pwr_dwn : tlv320aic33.h
- HPRCOM_is_constant_VCM : tlv320aic33.h
- HPRCOM_is_differential_of_HPLCOM : tlv320aic33.h
- HPRCOM_is_differential_of_HPROUT : tlv320aic33.h
- HPRCOM_is_external_feedback_with_HPLCOM_as_VCM_output : tlv320aic33.h
- HPRCOM_is_single_ended : tlv320aic33.h
- HPROUT_is_3_stated_with_pwr_dwn : tlv320aic33.h
- HPROUT_is_weakly_driven_to_common_mode_when_pwr_dwn : tlv320aic33.h
- HW_BRIDGE_UNIPROT_STATE_FAILED_TO_READ_METADATA : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_REQUEST_GET_METADATA : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_REQUEST_GET_NUM_OF_DEV : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_REQUEST_GET_SETTING : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_REQUEST_SET_SETTINGS : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_SEND_ONLY_RETURN_CODE : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_SEND_RETURN_CODE_AND_METADATA : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_SEND_RETURN_CODE_AND_SETTING : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_WAITING_FOR_REQUEST : HW_bridge_uniprot.h

### - i -

- if_short_protect_en_limit_max_current : tlv320aic33.h
- if_short_protect_en_power_down_when_short : tlv320aic33.h
- int16_type : generic_driver.h
- int32_type : generic_driver.h
- int8_type : generic_driver.h
- int_type : generic_driver.h

### - l -

- LCD_5110_ERROR : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_ERROR_SPI_INVALID_PARAMETER : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_ERROR_TIMEOUT : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_OK : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- left_and_right_DAC_channels_independent_volume : tlv320aic33.h
- left_DAC_channel_follows_right_channel : tlv320aic33.h
- left_dac_datapath_is_off : tlv320aic33.h
- left_dac_datapath_plays_left_channel_input_data : tlv320aic33.h
- left_dac_datapath_plays_mono_mix_left_and_right_channel_input_data : tlv320aic33.h
- left_dac_datapath_plays_right_channel_input_data : tlv320aic33.h
- left_DAC_output_DAC_L1_path : tlv320aic33.h
- left_DAC_output_DAC_L2_path : tlv320aic33.h
- left_DAC_output_DAC_L3_path : tlv320aic33.h

### - n -

- not_all_programmed_gains_to_HPLOUT_have_been_applied_yet : tlv320aic33.h
- not_all_programmed_gains_to_HPROUT_have_been_applied_yet : tlv320aic33.h

### - p -

- PLLCLK_IN_uses_BLCK : tlv320aic33.h
- PLLCLK_IN_uses_GPIO2 : tlv320aic33.h
- PLLCLK_IN_uses_MCLK : tlv320aic33.h

### - r -

- re_sync_with_soft_muting : tlv320aic33.h
- re_sync_without_soft_muting : tlv320aic33.h
- right_DAC_channel_follows_left_channel : tlv320aic33.h
- right_dac_datapath_is_off : tlv320aic33.h
- right_dac_datapath_plays_left_channel_input_data : tlv320aic33.h
- right_dac_datapath_plays_mono_mix_left_and_right_channel_input_data : tlv320aic33.h
- right_dac_datapath_plays_right_channel_input_data : tlv320aic33.h
- right_DAC_output_DAC_R1_path : tlv320aic33.h
- right_DAC_output_DAC_R2_path : tlv320aic33.h
- right_DAC_output_DAC_R3_path : tlv320aic33.h

### - s -

- serial_data_bus_uses_DSP_mode : tlv320aic33.h
- serial_data_bus_uses_I2S_mode : tlv320aic33.h
- serial_data_bus_uses_left_justified_mode : tlv320aic33.h
- serial_data_bus_uses_right_justified_mode : tlv320aic33.h

### - t -

- three_state_DOUT_when_valid_data_is_not_being_send : tlv320aic33.h
- TLV320AIC33_ERROR : tlv320aic33_HAL_AVR32_UC3A3_HW_interface.h
- TLV320AIC33_ERROR_TWI_INVALID_PARAMETER : tlv320aic33_HAL_AVR32_UC3A3_HW_interface.h
- TLV320AIC33_ERROR_TWI_NACK : tlv320aic33_HAL_AVR32_UC3A3_HW_interface.h
- TLV320AIC33_ERROR_TWI_TIMEOUT : tlv320aic33_HAL_AVR32_UC3A3_HW_interface.h
- TLV320AIC33_OK : tlv320aic33_HAL_AVR32_UC3A3_HW_interface.h

### - u -

- uint16_type : generic_driver.h
- uint32_type : generic_driver.h
- uint8_type : generic_driver.h
- uint_type : generic_driver.h
- UNI_FAIL : uniprot.h
- UNI_INVALID_PARAMETER : uniprot.h
- UNI_STATE_CMD_CHAR : uniprot.h
- UNI_STATE_CMD_CRC16_H : uniprot.h
- UNI_STATE_CMD_CRC16_L : uniprot.h
- UNI_STATE_CRC16_H : uniprot.h
- UNI_STATE_CRC16_L : uniprot.h
- UNI_STATE_DATA : uniprot.h
- UNI_STATE_DATA_D : uniprot.h
- UNI_STATE_HEADER_H : uniprot.h
- UNI_STATE_HEADER_NOB_H : uniprot.h
- UNI_STATE_HEADER_NOB_L : uniprot.h
- UNI_STATE_TAIL_T : uniprot.h
- UNI_SUCCESS : uniprot.h
- UNI_TX_PACKET_NOT_CONFIGURED : uniprot.h

### - v -

- void_type : generic_driver.h

### - w -

- word_clock_is_an_input : tlv320aic33.h
- word_clock_is_an_output : tlv320aic33.h