Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w
- x

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - a -

- adc_dual_rate_mode_is_disabled : tlv320aic33.h
- adc_dual_rate_mode_is_enabled : tlv320aic33.h
- AIA_INDEX : usb_descriptors.h
- AIN_INDEX : usb_descriptors.h
- AIT_INDEX : usb_descriptors.h
- AK5394A_pdca_disable() : taskAK5394A.c , taskAK5394A.h
- AK5394A_pdca_enable() : taskAK5394A.c , taskAK5394A.h
- AK5394A_task_init() : taskAK5394A.c , taskAK5394A.h
- all_programmed_gains_to_HPLOUT_have_been_applied_yet : tlv320aic33.h
- all_programmed_gains_to_HPROUT_have_been_applied_yet : tlv320aic33.h
- ALT0_AS_INTERFACE_CLASS : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- ALT0_AS_INTERFACE_INDEX : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- ALT0_AS_INTERFACE_PROTOCOL : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- ALT0_AS_INTERFACE_SUB_CLASS : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- ALT0_AS_NB_ENDPOINT : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- ALT1_AS_INTERFACE_CLASS : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- ALT1_AS_INTERFACE_INDEX : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- ALT1_AS_INTERFACE_PROTOCOL : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- ALT1_AS_INTERFACE_SUB_CLASS : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- ALT1_AS_NB_ENDPOINT : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- ALT1_AS_NB_ENDPOINT_OUT : uac2_usb_descriptors.h
- ALT2_AS_INTERFACE_CLASS : uac2_usb_descriptors.h
- ALT2_AS_INTERFACE_INDEX : uac2_usb_descriptors.h
- ALT2_AS_INTERFACE_PROTOCOL : uac2_usb_descriptors.h
- ALT2_AS_INTERFACE_SUB_CLASS : uac2_usb_descriptors.h
- ALT2_AS_NB_ENDPOINT : uac2_usb_descriptors.h
- ALTERNATE_NB0 : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- ALTERNATE_NB1 : uac2_usb_descriptors.h
- ALTERNATE_NB2 : uac1_usb_descriptors.h
- AOT_INDEX : usb_descriptors.h
- AS_CHAN_CONFIG : uac2_usb_descriptors.h
- AS_CONTROLS : uac2_usb_descriptors.h
- AS_DELAY : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- AS_FORMAT_TAG : uac1_usb_descriptors.h
- AS_FORMAT_TYPE : uac2_usb_descriptors.h
- AS_FORMATS : uac2_usb_descriptors.h
- AS_NB_CHANNELS : uac2_usb_descriptors.h
- AS_TERMINAL_LINK : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- AS_TERMINAL_LINK_OUT : uac2_usb_descriptors.h
- audio_buffer_0 : sync_control.h , taskAK5394A.c , taskAK5394A.h
- audio_buffer_1 : sync_control.h , taskAK5394A.h , taskAK5394A.c
- audio_buffer_in : taskAK5394A.h , taskAK5394A.c , sync_control.h
- audio_buffer_out : uac1_device_audio_task.c , uac2_device_audio_task.c
- audio_buffer_ptr : uac1_device_audio_task.c
- AUDIO_BUFFER_SIZE : taskAK5394A.h , sync_control.h
- AUDIO_CLASS_REVISION : uac1_usb_descriptors.h
- AUDIO_CLASS_REVISION_2 : uac2_usb_descriptors.h
- audio_connected : host_audio_task.c
- audio_cpt_sof : host_audio_task.c
- audio_data_word_length_16bit : tlv320aic33.h
- audio_data_word_length_20bit : tlv320aic33.h
- audio_data_word_length_24bit : tlv320aic33.h
- audio_data_word_length_32bit : tlv320aic33.h
- AUDIO_EP_ATRIBUTES : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- AUDIO_EP_CONTROLS : uac2_usb_descriptors.h
- AUDIO_EP_DELAY_UNIT : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- AUDIO_EP_LOCK_DELAY : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- audio_new_device_connected : host_audio_task.c
- AUDIO_PRODUCT_ID_1 : usb_descriptors.h
- AUDIO_PRODUCT_ID_2 : usb_descriptors.h
- AUDIO_VENDOR_ID : usb_descriptors.h