Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w
- x

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - c -

- cdc_get_line_coding() : usb_specific_request.h
- cdc_set_control_line_state() : usb_specific_request.h
- cdc_set_line_coding() : usb_specific_request.h
- char_type : generic_driver.h
- CLKDIV_IN_uses_BCLK : tlv320aic33.h
- CLKDIV_IN_uses_GPIO2 : tlv320aic33.h
- CLKDIV_IN_uses_MCLK : tlv320aic33.h
- clock_256_transfer_mode : tlv320aic33.h
- clock_changed : usb_specific_request.c , usb_specific_request.h
- clock_selected : usb_specific_request.c , usb_specific_request.h
- CLOCK_SELECTOR_INDEX : usb_descriptors.h
- CLOCK_SOURCE_1_INDEX : usb_descriptors.h
- CLOCK_SOURCE_2_INDEX : usb_descriptors.h
- common_output_voltage_generated_from_bandgap_reference : tlv320aic33.h
- common_output_voltage_generated_from_resistor_divider : tlv320aic33.h
- CONF_ATTRIBUTES : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- CONF_INDEX : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- CONF_NB : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- configTSK_USB_DEV_PERIOD : usb_descriptors.c , usb_descriptors.h
- continuous_transfer_mode : tlv320aic33.h
- COUNTER_TIME_OUT : composite_widget.h
- cs2200_calc_frequency() : cs2200.c , cs2200.h
- cs2200_calc_ratio() : cs2200.c , cs2200.h
- CS2200_config_table : cs2200.c , cs2200.h
- cs2200_dec_PLL_freq() : cs2200.c , cs2200.h
- cs2200_disable_device_cfg() : cs2200.c , cs2200.h
- cs2200_enable_device_cfg() : cs2200.c , cs2200.h
- CS2200_ERROR : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_ERROR_TWI_INVALID_PARAMETER : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_ERROR_TWI_NACK : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_ERROR_TWI_TIMEOUT : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- cs2200_get_freeze_bit() : cs2200.c , cs2200.h
- cs2200_get_in_divider() : cs2200.c , cs2200.h
- cs2200_get_out_divider_multiplier() : cs2200.c , cs2200.h
- cs2200_get_out_divider_multiplier_float() : cs2200.c , cs2200.h
- cs2200_get_PLL_freq() : cs2200.c , cs2200.h
- cs2200_get_ratio() : cs2200.c , cs2200.h
- cs2200_get_save_change_ratio_by_1() : cs2200.c , cs2200.h
- cs2200_HAL_init() : cs2200_HAL_AVR32_UC3A3_HW_interface.c , cs2200_HAL_AVR32_UC3A3_HW_interface.h
- cs2200_HAL_read_data() : cs2200_HAL_AVR32_UC3A3_HW_interface.c , cs2200_HAL_AVR32_UC3A3_HW_interface.h
- cs2200_HAL_write_data() : cs2200_HAL_AVR32_UC3A3_HW_interface.c , cs2200_HAL_AVR32_UC3A3_HW_interface.h
- cs2200_in_div_t : cs2200.h
- cs2200_inc_PLL_freq() : cs2200.c , cs2200.h
- cs2200_init() : cs2200.c , cs2200.h
- CS2200_INPUT_DIVIDER_1x : cs2200.h
- CS2200_INPUT_DIVIDER_2x : cs2200.h
- CS2200_INPUT_DIVIDER_4x : cs2200.h
- CS2200_LOCK_TWI_MODULE_IF_RTOS : cs2200.h
- CS2200_MAP_AUTO_INC_BIT : cs2200.h
- CS2200_MAX_CMD_ID : cs2200.c
- CS2200_metadata : cs2200.c , cs2200.h
- CS2200_OK : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_R_MOD__DIV_16x : cs2200.h
- CS2200_R_MOD__DIV_2x : cs2200.h
- CS2200_R_MOD__DIV_4x : cs2200.h
- CS2200_R_MOD__DIV_8x : cs2200.h
- CS2200_R_MOD__MUL_1x : cs2200.h
- CS2200_R_MOD__MUL_2x : cs2200.h
- CS2200_R_MOD__MUL_4x : cs2200.h
- CS2200_R_MOD__MUL_8x : cs2200.h
- cs2200_r_mod_t : cs2200.h
- cs2200_read_data() : cs2200.h , cs2200.c
- CS2200_REF_CLK_FREQ : cs2200.h
- CS2200_REG_DEVICE_CFG_1 : cs2200.h
- CS2200_REG_DEVICE_CTRL : cs2200.h
- CS2200_REG_DEVICE_ID : cs2200.h
- CS2200_REG_FUNC_CFG_1 : cs2200.h
- CS2200_REG_FUNC_CFG_2 : cs2200.h
- CS2200_REG_GLOBAL_CFG : cs2200.h
- CS2200_REG_RATIO : cs2200.h
- CS2200_RTOS_CREATE_MUTEX : cs2200.h
- cs2200_set_freeze_bit() : cs2200.h , cs2200.c
- cs2200_set_in_divider() : cs2200.c , cs2200.h
- cs2200_set_out_divider_multiplier() : cs2200.h , cs2200.c
- cs2200_set_out_divider_multiplier_float() : cs2200.c , cs2200.h
- cs2200_set_PLL_freq() : cs2200.h , cs2200.c
- cs2200_set_ratio() : cs2200.h , cs2200.c
- cs2200_set_save_change_ratio_by_1() : cs2200.h , cs2200.c
- cs2200_status_t : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_SUPPORT_GENERIC_DRIVER : cs2200.h
- CS2200_SUPPORT_RTOS : cs2200.h
- CS2200_TWI_ADDRESS : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_TWI_BAUDRATE : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_TWI_CKDIV : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_TWI_CLDIV : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_TWI_CLK_SOURCE : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_TWI_DEVICE : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_TWI_SCL_FUNCTION : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_TWI_SCL_PIN : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_TWI_SDA_FUNCTION : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_TWI_SDA_PIN : cs2200_HAL_AVR32_UC3A3_HW_interface.h
- CS2200_TWI_TIMEOUT : cs2200_HAL_AVR32_UC3A3_HW_interface.c
- CS2200_UNLOCK_TWI_MODULE_IF_RTOS : cs2200.h
- cs2200_write_data() : cs2200.c , cs2200.h
- CSD_ID_1 : uac2_usb_descriptors.h
- CSD_ID_1_CONTROL : uac2_usb_descriptors.h
- CSD_ID_1_TYPE : uac2_usb_descriptors.h
- CSD_ID_2 : uac2_usb_descriptors.h
- CSD_ID_2_CONTROL : uac2_usb_descriptors.h
- CSD_ID_2_TYPE : uac2_usb_descriptors.h
- CSX_CONTROL : uac2_usb_descriptors.h
- CSX_ID : uac2_usb_descriptors.h
- CSX_INPUT_PINS : uac2_usb_descriptors.h
- CSX_SOURCE_1 : uac2_usb_descriptors.h
- CSX_SOURCE_2 : uac2_usb_descriptors.h
- current_freq : usb_specific_request.h , usb_specific_request.c