Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
cs2200_reg_img_t Struct Reference

Register image of CS2200. More...

`#include <cs2200.h>`

## Data Fields
union {
uint8_t device_id_reg
device_id_t Device_id
}; |
union {
uint8_t device_crtl_reg
device_ctrl_t Device_Ctrl
}; |
union {
uint8_t device_cfg_1_reg
device_Cfg_1_t Device_Cfg_1
}; |
union {
uint8_t global_cfg_reg
global_Cfg_t Global_Cfg
}; |
cs2200_32b_to_8b_t | Ratio
union {
uint8_t func_cfg_1_reg
func_Cfg_1_t Func_Cfg_1
}; |
union {
uint8_t func_cfg_2_reg
func_Cfg_2_t Func_Cfg_2
}; |

## Detailed Description

Register image of CS2200.

Because in one register is many independent bits, we must know every
single bit state when writing value to CS2200's register. So for this is
there this image which help keep collected data.

## Field Documentation

union { ... }

union { ... }

union { ... }

union { ... }

union { ... }

union { ... }

device_Cfg_1_t cs2200_reg_img_t::Device_Cfg_1

uint8_t cs2200_reg_img_t::device_cfg_1_reg

uint8_t cs2200_reg_img_t::device_crtl_reg

device_ctrl_t cs2200_reg_img_t::Device_Ctrl

device_id_t cs2200_reg_img_t::Device_id

uint8_t cs2200_reg_img_t::device_id_reg

func_Cfg_1_t cs2200_reg_img_t::Func_Cfg_1

uint8_t cs2200_reg_img_t::func_cfg_1_reg

func_Cfg_2_t cs2200_reg_img_t::Func_Cfg_2

uint8_t cs2200_reg_img_t::func_cfg_2_reg

global_Cfg_t cs2200_reg_img_t::Global_Cfg

uint8_t cs2200_reg_img_t::global_cfg_reg

cs2200_32b_to_8b_t cs2200_reg_img_t::Ratio

The documentation for this struct was generated from the following file:

- /mnt/data/GENTOO_FILES/home/k1ll3r/Dokumenty/Diplomka/Sonochan_II/FW_sdr_widget/sdr-widget/src/cs2200.h