Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w
- x

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - s -

- s_brd_drv_mute : brd_driver_hw_03.c
- s_brd_drv_pure_i2s_dir : brd_driver_hw_03.c
- s_brd_drv_rst_i2s : brd_driver_hw_03.c
- s_packet_cfg : uniprot.c
- s_register_img : cs2200.c
- s_status_reg : uniprot.c
- s_virtual_reg_img : tlv320aic33.c , cs2200.c
- SEND_BREAK : usb_specific_request.h
- SEND_ENCAPSULATED_COMMAND : usb_specific_request.h
- serial_data_bus_uses_DSP_mode : tlv320aic33.h
- serial_data_bus_uses_I2S_mode : tlv320aic33.h
- serial_data_bus_uses_left_justified_mode : tlv320aic33.h
- serial_data_bus_uses_right_justified_mode : tlv320aic33.h
- SET_CONTROL_LINE_STATE : usb_specific_request.h
- SET_LINE_CODING : usb_specific_request.h
- SN_INDEX : usb_descriptors.h
- speed : uac1_usb_specific_request.c
- Speedx_1 : uac2_usb_specific_request.c
- Speedx_2 : uac2_usb_specific_request.c
- SPK_ALT1_AS_NB_ENDPOINT : uac1_usb_descriptors.h
- SPK_AS_DELAY : uac1_usb_descriptors.h
- SPK_AS_FORMAT_TAG : uac1_usb_descriptors.h
- SPK_AS_TERMINAL_LINK : uac1_usb_descriptors.h
- SPK_BMA_CONTROLS : uac2_usb_descriptors.h
- SPK_BMA_CONTROLS_CH_1 : uac2_usb_descriptors.h
- SPK_BMA_CONTROLS_CH_2 : uac2_usb_descriptors.h
- spk_buffer_0 : sync_control.h , taskAK5394A.c , taskAK5394A.h
- spk_buffer_1 : taskAK5394A.c , taskAK5394A.h , sync_control.h
- spk_buffer_in : uac1_device_audio_task.c , uac2_device_audio_task.c
- spk_buffer_out : sync_control.h , taskAK5394A.c , taskAK5394A.h
- SPK_BUFFER_SIZE : sync_control.h , taskAK5394A.h
- SPK_FEATURE_UNIT_BMA_CONTROLS_0 : uac1_usb_descriptors.h
- SPK_FEATURE_UNIT_BMA_CONTROLS_1 : uac1_usb_descriptors.h
- SPK_FEATURE_UNIT_BMA_CONTROLS_2 : uac1_usb_descriptors.h
- SPK_FEATURE_UNIT_CH_NAME_ID : uac1_usb_descriptors.h
- SPK_FEATURE_UNIT_CONTROL_SIZE : uac1_usb_descriptors.h
- SPK_FEATURE_UNIT_ID : uac2_usb_descriptors.h , uac1_usb_descriptors.h
- SPK_FEATURE_UNIT_SOURCE_ID : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- spk_index : uac1_device_audio_task.c , uac2_device_audio_task.c
- SPK_INPUT_TERMINAL_ASSOCIATION : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- SPK_INPUT_TERMINAL_CH_NAME_ID : uac2_usb_descriptors.h , uac1_usb_descriptors.h
- SPK_INPUT_TERMINAL_CHANNEL_CONF : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- SPK_INPUT_TERMINAL_ID : uac2_usb_descriptors.h , uac1_usb_descriptors.h
- SPK_INPUT_TERMINAL_NB_CHANNELS : uac2_usb_descriptors.h , uac1_usb_descriptors.h
- SPK_INPUT_TERMINAL_TYPE : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- spk_mute : device_audio_task.c , device_audio_task.h
- SPK_OUTPUT_TERMINAL_ASSOCIATION : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- SPK_OUTPUT_TERMINAL_CONTROLS : uac2_usb_descriptors.h
- SPK_OUTPUT_TERMINAL_ID : uac2_usb_descriptors.h , uac1_usb_descriptors.h
- SPK_OUTPUT_TERMINAL_SOURCE_ID : uac2_usb_descriptors.h , uac1_usb_descriptors.h
- SPK_OUTPUT_TERMINAL_TYPE : uac2_usb_descriptors.h , uac1_usb_descriptors.h
- SPK_PDCA_OPTIONS : taskAK5394A.c
- spk_volume : device_audio_task.h , device_audio_task.c
- ssc : taskAK5394A.c , taskAK5394A.h , sync_control.h
- SSC_GPIO_MAP : taskAK5394A.c
- STARTUP_LED_DELAY : uac1_device_audio_task.c , uac2_device_audio_task.c
- STD_AS_INTERFACE_IN : uac1_usb_descriptors.h , uac2_usb_descriptors.h
- STD_AS_INTERFACE_OUT : uac1_usb_descriptors.h , uac2_usb_descriptors.h