Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
uac2_usb_specific_request.h File Reference
`#include "conf_usb.h"`

Go to the source code of this file.

## Functions
void | uac2_user_endpoint_init (U8)
| This function configures the endpoints of the device application. This function is called when the set configuration request has been received. More...
void | uac2_user_set_interface (U8 wIndex, U8 wValue)
| This function handles usb_set_interface side effects. This function is called from usb_set_interface in usb_standard_request in case there are side effects of the interface change to be handled. More...
Bool | uac2_user_read_request (U8, U8)