Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w
- x

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - h -

- HEADSET_CATEGORY : uac2_usb_descriptors.h
- HID_COUNTRY_CODE : uac1_usb_descriptors.h
- HID_NUM_DESCRIPTORS : uac1_usb_descriptors.h
- HID_VERSION : uac1_usb_descriptors.h
- host_audio_get_max() : host_audio_task.c , host_audio_task.h
- host_audio_set_cur() : host_audio_task.h , host_audio_task.c
- host_audio_set_cur_mute() : host_audio_task.c , host_audio_task.h
- host_audio_task() : host_audio_task.c , host_audio_task.h
- host_audio_task_init() : host_audio_task.c , host_audio_task.h
- host_set_sampling_rate() : host_audio_task.h , host_audio_task.c
- HPLCOM_is_constant_VCM : tlv320aic33.h
- HPLCOM_is_differential_of_HPLOUT : tlv320aic33.h
- HPLCOM_is_single_ended : tlv320aic33.h
- HPLOUT_is_3_stated_with_pwr_dwn : tlv320aic33.h
- HPLOUT_is_weakly_driven_to_common_mode_when_pwr_dwn : tlv320aic33.h
- HPRCOM_is_constant_VCM : tlv320aic33.h
- HPRCOM_is_differential_of_HPLCOM : tlv320aic33.h
- HPRCOM_is_differential_of_HPROUT : tlv320aic33.h
- HPRCOM_is_external_feedback_with_HPLCOM_as_VCM_output : tlv320aic33.h
- HPRCOM_is_single_ended : tlv320aic33.h
- HPROUT_is_3_stated_with_pwr_dwn : tlv320aic33.h
- HPROUT_is_weakly_driven_to_common_mode_when_pwr_dwn : tlv320aic33.h
- HW_BRIDGE_UNIPROT_DEBUG : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_RX_BUFFER_SIZE : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_FAILED_TO_READ_METADATA : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_REQUEST_GET_METADATA : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_REQUEST_GET_NUM_OF_DEV : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_REQUEST_GET_SETTING : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_REQUEST_SET_SETTINGS : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_SEND_ONLY_RETURN_CODE : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_SEND_RETURN_CODE_AND_METADATA : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_SEND_RETURN_CODE_AND_SETTING : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_STATE_WAITING_FOR_REQUEST : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_SUPPORT_RTOS : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_TX_BUFFER_SIZE : HW_bridge_uniprot.h
- HW_BRIDGE_UNIPROT_USED_PIPE : HW_bridge_uniprot.h
- hw_get_device_metadata() : HW.c , HW.h
- hw_get_max_device_index() : HW.c , HW.h
- hw_get_setting() : HW.c , HW.h
- HW_MAX_DEVICE_ID : HW.h
- HW_POINTER_ARRAY_TO_METADATA : HW.h
- hw_set_setting() : HW.h , HW.c