Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w
- x

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - l -

- LANG_ID : usb_descriptors.h
- LANGUAGE_ID : usb_descriptors.h
- LCD_5110_add_16bit_dec_unsigned_to_string() : LCD_5110.c
- LCD_5110_add_8bit_dec_unsigned_to_string() : LCD_5110.c
- LCD_5110_add_8bit_hex_to_sring() : LCD_5110.c
- LCD_5110_add_tens_to_string() : LCD_5110.c
- LCD_5110_add_unit_to_string() : LCD_5110.c
- LCD_5110_auto_clear_display() : LCD_5110.c , LCD_5110.h
- LCD_5110_auto_clear_line() : LCD_5110.c , LCD_5110.h
- LCD_5110_auto_newline() : LCD_5110.c , LCD_5110.h
- LCD_5110_backlight_off : LCD_5110.h
- LCD_5110_backlight_on : LCD_5110.h
- LCD_5110_clear() : LCD_5110.c , LCD_5110.h
- LCD_5110_clear_line() : LCD_5110.c , LCD_5110.h
- LCD_5110_CS_support : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_DEFAULT_AUTO_LCD_CLEAR : LCD_5110.h
- LCD_5110_DEFAULT_AUTO_LF : LCD_5110.h
- LCD_5110_DEFAULT_AUTO_LINE_CLEAR : LCD_5110.h
- LCD_5110_ERROR : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_ERROR_SPI_INVALID_PARAMETER : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_ERROR_TIMEOUT : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_font6x8 : LCD_5110.c
- LCD_5110_HAL_backlight_off() : LCD_5110_HAL_AVR32_UC3A3_HW_interface.c , LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_HAL_backlight_on() : LCD_5110_HAL_AVR32_UC3A3_HW_interface.c , LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_HAL_init() : LCD_5110_HAL_AVR32_UC3A3_HW_interface.c , LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_HAL_init_SPI() : LCD_5110_HAL_AVR32_UC3A3_HW_interface.c
- LCD_5110_HAL_send_command_byte() : LCD_5110_HAL_AVR32_UC3A3_HW_interface.c , LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_HAL_send_data_byte() : LCD_5110_HAL_AVR32_UC3A3_HW_interface.c , LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_HAL_wait_for_SPI_tx() : LCD_5110_HAL_AVR32_UC3A3_HW_interface.c
- LCD_5110_init() : LCD_5110.c , LCD_5110.h
- LCD_5110_IO_HIGH : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_IO_HIGH_simple : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_IO_LOW : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_IO_LOW_simple : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_LIGHT_PIN : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_LIGHT_support : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_LOCK_SPI_MODULE_IF_RTOS : LCD_5110.h
- LCD_5110_OK : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_RESET_NUM_OF_CYCLES : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_RESET_support : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_RST_PIN : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_RTOS_CREATE_MUTEX : LCD_5110.h
- LCD_5110_send_command_byte() : LCD_5110.c , LCD_5110.h
- LCD_5110_send_data_byte() : LCD_5110.c , LCD_5110.h
- LCD_5110_set_line() : LCD_5110.c , LCD_5110.h
- LCD_5110_set_X() : LCD_5110.c , LCD_5110.h
- LCD_5110_show_digit() : LCD_5110.c
- LCD_5110_SPI_BAUDRATE : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_BITS_PER_TRANSFER : LCD_5110_HAL_AVR32_UC3A3_HW_interface.c
- LCD_5110_SPI_CHIP_SELECT : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_CLK_SOURCE : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_CS_FUNCTION : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_CS_PIN : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_DC_PIN : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_DELAY_BETWEEN_CS : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_DELAY_CS_STOP : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_DELAY_SCK_START : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_DEVICE : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_MOSI_FUNCTION : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_MOSI_PIN : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_SCBR : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_SCK_FUNCTION : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_SCK_PIN : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SPI_TIMEOUT : LCD_5110_HAL_AVR32_UC3A3_HW_interface.h
- LCD_5110_SUPPORT_RTOS : LCD_5110.h
- LCD_5110_UNLOCK_SPI_MODULE_IF_RTOS : LCD_5110.h
- LCD_5110_write() : LCD_5110.h , LCD_5110.c
- LCD_5110_write_dec16_signed() : LCD_5110.h , LCD_5110.c
- LCD_5110_write_dec16_unsigned() : LCD_5110.h , LCD_5110.c
- LCD_5110_write_dec8_signed() : LCD_5110.h , LCD_5110.c
- LCD_5110_write_dec8_unsigned() : LCD_5110.c , LCD_5110.h
- LCD_5110_write_hex16() : LCD_5110.c , LCD_5110.h
- LCD_5110_write_hex32() : LCD_5110.c , LCD_5110.h
- LCD_5110_write_hex8() : LCD_5110.c , LCD_5110.h
- LCD_5110_write_to_line() : LCD_5110.h , LCD_5110.c
- LCD_5110_write_xy() : LCD_5110.c , LCD_5110.h
- left_and_right_DAC_channels_independent_volume : tlv320aic33.h
- left_DAC_channel_follows_right_channel : tlv320aic33.h
- left_dac_datapath_is_off : tlv320aic33.h
- left_dac_datapath_plays_left_channel_input_data : tlv320aic33.h
- left_dac_datapath_plays_mono_mix_left_and_right_channel_input_data : tlv320aic33.h
- left_dac_datapath_plays_right_channel_input_data : tlv320aic33.h
- left_DAC_output_DAC_L1_path : tlv320aic33.h
- left_DAC_output_DAC_L2_path : tlv320aic33.h
- left_DAC_output_DAC_L3_path : tlv320aic33.h