## This file is a general .ucf for Nexys3 rev B board
## To use it in a project:
## - remove or comment the lines corresponding to unused pins
## - rename the used signals according to the project

##Clock signal
Net "clk" LOC=V10 | IOSTANDARD=LVCMOS33;
#Net "clk" TNM_NET = sys_clk_pin;
#TIMESPEC TS_sys_clk_pin = PERIOD sys_clk_pin 100000 kHz;

## onBoard USB controller
#Net "EppAstb" LOC = H1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L41N_GCLK26_M3DQ5, Sch name = U-FLAGA
#Net "EppDstb" LOC = K4 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L42P_GCLK25_TRDY2_M3UDM, Sch name = U-FLAGB
#Net "EppWait" LOC = C2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L83P, Sch name = U-SLRD
#Net "EppDB<0>" LOC = E1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L50N_M3BA2, Sch name = U-FD0
#Net "EppDB<1>" LOC = F4 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L51P_M3A10, Sch name = U-FD1
#Net "EppDB<2>" LOC = F3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L51N_M3A4, Sch name = U-FD2
#Net "EppDB<3>" LOC = D2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L52P_M3A8, Sch name = U-FD3
#Net "EppDB<4>" LOC = D1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L52N_M3A9, Sch name = U-FD4
#Net "EppDB<5>" LOC = H7 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L53P_M3CKE, Sch name = U-FD5
#Net "EppDB<6>" LOC = G6 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L53N_M3A12, Sch name = U-FD6
#Net "EppDB<7>" LOC = E4 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L54P_M3RESET, Sch name = U-FD7

#Net "UsbClk" LOC = H2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L41P_GCLK27_M3DQ4, Sch name = U-IFCLK
#Net "UsbDir" LOC = F6 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L55P_M3A13, Sch name = U-SLCS

#Net "UsbWR" LOC = C1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L83N_VREF, Sch name = U-SLWR
#Net "UsbOE" LOC = H6 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L49P_M3A7, Sch name = U-SLOE

#Net "UsbAdr<1>" LOC = E3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L50P_M3WE, Sch name = U-FIFOAD1
#Net "UsbAdr<0>" LOC = H5 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L49N_M3A2, Sch name = U-FIFOAD0

#Net "UsbPktend" LOC = D3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L54N_M3A11, Sch name = U-PKTEND

#Net "UsbFlag" LOC = F5 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L55N_M3A14, Sch name = U-FLAGC
#Net "UsbMode" LOC = F1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L48N_M3BA1, Sch name = U-INT0#

## onBoard Cellular RAM, Numonyx StrataFlash and Numonyx Quad Flash
#Net "MemOE" LOC = L18 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L46N_FOE_B_M1DQ3, Sch name = P30-OE
#Net "MemWR" LOC = M16 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L47P_FWE_B_M1DQ0, Sch name = P30-WE
#Net "MemAdv" LOC = H18 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L43N_GCLK4_M1DQ5, Sch name = P30-ADV
#Net "MemWait" LOC = V4 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L63N, Sch name = P30-WAIT
#Net "MemClk" LOC = R10 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L29P_GCLK3, Sch name = P30-CLK

#Net "RamCS" LOC = L15 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L42P_GCLK7_M1UDM, Sch name = MT-CE
#Net "RamCRE" LOC = M18 |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L47N_LDC_M1DQ1, Sch name = MT-CRE
#Net "RamUB" LOC = K15  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L41P_GCLK9_IRDY1_M1RASN, Sch name = MT-UB
#Net "RamLB" LOC = K16  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L41N_GCLK8_M1CASN, Sch name = MT-LB

#Net "FlashCS" LOC = L17 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L46P_FCS_B_M1DQ2, Sch name = P30-CE
#Net "FlashRp" LOC = T4  | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L63P, Sch name = P30-RST

#Net "QuadSpiFlashCS" LOC = V3  | IOSTANDARD = LVCMOS33; #Bank = MISC, pin name = IO_L65N_CSO_B_2, Sch name = CS
#Net "QuadSpiFlashSck"  LOC = R15 | IOSTANDARD = LVCMOS33; #Bank = MISC, pin name = IO_L1P_CCLK_2, Sch name = SCK

#Net "MemAdr<1>" LOC = K18  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L45N_A0_M1LDQSN, Sch name = P30-A0
#Net "MemAdr<2>" LOC = K17  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L45P_A1_M1LDQS, Sch name = P30-A1
#Net "MemAdr<3>" LOC = J18  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L44N_A2_M1DQ7, Sch name = P30-A2
#Net "MemAdr<4>" LOC = J16  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L44P_A3_M1DQ6, Sch name = P30-A3
#Net "MemAdr<5>" LOC = G18  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L38N_A4_M1CLKN, Sch name = P30-A4
#Net "MemAdr<6>" LOC = G16  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L38P_A5_M1CLK, Sch name = P30-A5
#Net "MemAdr<7>" LOC = H16  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L37N_A6_M1A1, Sch name = P30-A6
#Net "MemAdr<8>" LOC = H15  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L37P_A7_M1A0, Sch name = P30-A7
#Net "MemAdr<9>" LOC = H14  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L36N_A8_M1BA1, Sch name = P30-A8
#Net "MemAdr<10>" LOC = H13  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L36P_A9_M1BA0, Sch name = P30-A9
#Net "MemAdr<11>" LOC = F18  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L35N_A10_M1A2, Sch name = P30-A10
#Net "MemAdr<12>" LOC = F17  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L35P_A11_M1A7, Sch name = P30-A11
#Net "MemAdr<13>" LOC = K13  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L34N_A12_M1BA2, Sch name = P30-A12
#Net "MemAdr<14>" LOC = K12  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L34P_A13_M1WE, Sch name = P30-A13
#Net "MemAdr<15>" LOC = E18  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L33N_A14_M1A4, Sch name = P30-A14
#Net "MemAdr<16>" LOC = E16  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L33P_A15_M1A10, Sch name = P30-A15
#Net "MemAdr<17>" LOC = G13  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L32N_A16_M1A9, Sch name = P30-A16
#Net "MemAdr<18>" LOC = H12  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L32P_A17_M1A8, Sch name = P30-A17
#Net "MemAdr<19>" LOC = D18  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L31N_A18_M1A12, Sch name = P30-A18
#Net "MemAdr<20>" LOC = D17  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L31P_A19_M1CKE, Sch name = P30-A19
#Net "MemAdr<21>" LOC = G14  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L30N_A20_M1A11, Sch name = P30-A20
#Net "MemAdr<22>" LOC = F14  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L30P_A21_M1RESET Sch name = P30-A21
#Net "MemAdr<23>" LOC = C18  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L29N_A22_M1A14, Sch name = P30-A22
#Net "MemAdr<24>" LOC = C17  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L29P_A23_M1A13, Sch name = P30-A23
#Net "MemAdr<25>" LOC = F16  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L1N_A24_VREF, Sch name = P30-A24
#Net "MemAdr<26>" LOC = F15  |  IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L1P_A25, Sch name = P30-A25

#Net "QuadSpiFlashDB<0>" LOC = T13 |  IOSTANDARD = LVCMOS33; #Dual/Quad SPI Flash DB<0>, Bank = MISC, pin name = IO_L3N_MOSI_CSI_B_MISO0_2, Sch name = SDI
#Net "MemDB<0>" LOC = R13 |  IOSTANDARD = LVCMOS33; #Ram or Numonyx Paralell Flash DB<0>, or Dual/Quad SPI Flash DB<1>, Bank = MISC, pin name = IO_L3P_D0_DIN_MISO_MISO1_2, Sch name = P30-DQ0
#Net "MemDB<1>" LOC = T14 |  IOSTANDARD = LVCMOS33; #Ram or Numonyx Paralell Flash DB<1>, or Quad SPI Flash DB<2>, Bank = MISC, pin name = IO_L12P_D1_MISO2_2, Sch name = P30-DQ1
#Net "MemDB<2>" LOC = V14 |  IOSTANDARD = LVCMOS33; #Ram or Numonyx Paralell Flash DB<2>, or Quad SPI Flash DB<3>, Bank = MISC, pin name = IO_L12N_D2_MISO3_2, Sch name = P30-DQ2
#Net "MemDB<3>" LOC = U5  |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_49P_D3, Sch name = P30-DQ3
#Net "MemDB<4>" LOC = V5  |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_49N_D4, Sch name = P30-DQ4
#Net "MemDB<5>" LOC = R3  |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L62P_D5, Sch name = P30-DQ5
#Net "MemDB<6>"  LOC = T3  |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L62N_D6, Sch name = P30-DQ6
#Net "MemDB<7>"  LOC = R5  |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L48P_D7, Sch name = P30-DQ7
#Net "MemDB<8>"  LOC = N5  |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L64P_D8, Sch name = P30-DQ8
#Net "MemDB<9>"  LOC = P6  |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L64N_D9, Sch name = P30-DQ9
#Net "MemDB<10>"  LOC = P12 |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L13N_D10, Sch name = P30-DQ10
#Net "MemDB<11>"  LOC = U13 |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L14P_D11, Sch name = P30-DQ11
#Net "MemDB<12>"  LOC = V13 |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L14N_D12, Sch name = P30-DQ12
#Net "MemDB<13>"  LOC = U10 |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L30P_GCLK1_D13, Sch name = P30-DQ13
#Net "MemDB<14>"  LOC = R8  |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L31P_GCLK31_D14, Sch name = P30-DQ14
#Net "MemDB<15>"  LOC = T8  |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L31N_GCLK30_D15, Sch name = P30-DQ15

## SMSC ethernet PHY
#Net "PhyRstn" LOC = P3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L2N, Sch name = ETH-RST
#Net "PhyCrs" LOC = N3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L1N_VREF, Sch name = ETH-CRS
#Net "PhyCol" LOC = P4 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L2P, Sch name = ETH-COL
#Net "PhyClk25Mhz" LOC = N4 | IOSTANDARD = LVCMOS33; #Unconnected if R172 is not loaded, Bank = 3, pin name = IO_L1P, Sch name = ETH-CLK25MHZ

#Net "PhyTxd<3>" LOC = T1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L33N_M3DQ13, Sch name = ETH-TXD3 
#Net "PhyTxd<2>" LOC  = T2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L33P_M3DQ12, Sch name = ETH-TXD2
#Net "PhyTxd<1>" LOC = U1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L32N_M3DQ15, Sch name = ETH-TXD1
#Net "PhyTxd<0>" LOC = U2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L32P_M3DQ14, Sch name = ETH-TXD0
#Net "PhyTxEn" LOC = L2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L37P_M3DQ0, Sch name = ETH-TX_EN
#Net "PhyTxClk" LOC = L5 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L43P_GCLK23_M3RASN, Sch name = ETH-TX_CLK
#Net "PhyTxEr" LOC = P2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L34P_M3UDQS, Sch name = ETH-TXD4

#Net "PhyRxd<3>" LOC = M3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L36P_M3DQ8, Sch name = ETH-RXD3
#Net "PhyRxd<2>" LOC = N1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L35N_M3DQ11, Sch name = ETH-RXD2
#Net "PhyRxd<1>" LOC = N2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L35P_M3DQ10, Sch name = ETH-RXD1
#Net "PhyRxd<0>" LOC = P1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L34N_M3UDQSN, Sch name = ETH-RXD0
#Net "PhyRxDv" LOC = L1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L37N_M3DQ1, Sch name = ETH-RX_DV
#Net "PhyRxEr" LOC = M1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L36N_M3DQ9, Sch name = ETH-RXD4
#Net "PhyRxClk" LOC = H4 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L44P_GCLK21_M3A5, Sch name = ETH-RX_CLK

#Net "PhyMdc" LOC = M5 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L31N_VREF, Sch name = ETH-MDC
#Net "PhyMdio" LOC = L6 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L31P, Sch name = ETH-MDIO

## Pic USB-HID interface
#Net "PS2KeyboardData" LOC = J13| IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L39P_M1A3, Sch name = PIC-SDI1
#Net "PS2KeyboardClk" LOC = L12 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L40P_GCLK11_M1A5, Sch name = PIC-SCK1

#NET "PS2MouseData" LOC = K14 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L39N_M1ODT, Sch name = PIC-SDO1
#NET "PS2MouseClk" LOC = L13| IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L40N_GCLK10_M1A6, Sch name = PIC-SS1

#Net "PicGpio<0>" LOC = L16 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L42N_GCLK6_TRDY1_M1LDM, Sch name = PIC-GPIO0
#NET "PicGpio<1>" LOC = H17 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L43P_GCLK5_M1DQ4, Sch name = PIC-GPIO1

## Usb-RS232 interface
#Net "RxD" LOC = N17 | IOSTANDARD=LVCMOS33; #Bank = 1, pin name = IO_L48P_HDC_M1DQ8, Sch name = MCU-RX
#Net "TxD" LOC = N18 | IOSTANDARD=LVCMOS33; #Bank = 1, pin name = IO_L48N_M1DQ9, Sch name = MCU-TX

## 7 segment display
Net "seg<0>" LOC = T17 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L51P_M1DQ12, Sch name = CA
Net "seg<1>" LOC = T18 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L51N_M1DQ13, Sch name = CB
Net "seg<2>" LOC = U17 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L52P_M1DQ14, Sch name = CC
Net "seg<3>" LOC = U18 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L52N_M1DQ15, Sch name = CD
Net "seg<4>" LOC = M14 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L53P, Sch name = CE
Net "seg<5>" LOC = N14 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L53N_VREF, Sch name = CF
Net "seg<6>" LOC = L14 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L61P, Sch name = CG
#Net "seg<7>" LOC = M13 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L61N, Sch name = DP

Net "an<0>" LOC = N16 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L50N_M1UDQSN, Sch name = AN0
Net "an<1>" LOC = N15 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L50P_M1UDQS, Sch name = AN1
Net "an<2>" LOC = P18 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L49N_M1DQ11, Sch name = AN2
Net "an<3>" LOC = P17 | IOSTANDARD = LVCMOS33; #Bank = 1, pin name = IO_L49P_M1DQ10, Sch name = AN3

## Leds
#Net "Led<0>" LOC = U16 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L2P_CMPCLK, Sch name = LD0
#Net "Led<1>" LOC = V16 |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L2N_CMPMOSI, Sch name = LD1
#Net "Led<2>" LOC = U15 |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L5P, Sch name = LD2
#Net "Led<3>" LOC = V15 |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L5N, Sch name = LD3
#Net "Led<4>" LOC = M11 |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L15P, Sch name = LD4
#Net "Led<5>" LOC = N11 |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L15N, Sch name = LD5
#Net "Led<6>" LOC = R11 |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L16P, Sch name = LD6
#Net "Led<7>" LOC = T11 |  IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L16N_VREF, Sch name = LD7

## Switches
#Net "sw<0>" LOC = T10 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L29N_GCLK2, Sch name = SW0
#Net "sw<1>" LOC = T9 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L32P_GCLK29, Sch name = SW1
#Net "sw<2>" LOC = V9 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L32N_GCLK28, Sch name = SW2
#Net "sw<3>" LOC = M8 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L40P, Sch name = SW3
#Net "sw<4>" LOC = N8 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L40N, Sch name = SW4
#Net "sw<5>" LOC = U8 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L41P, Sch name = SW5
#Net "sw<6>" LOC = V8 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L41N_VREF, Sch name = SW6
#Net "sw<7>" LOC = T5 | IOSTANDARD = LVCMOS33; #Bank = MISC, pin name = IO_L48N_RDWR_B_VREF_2, Sch name = SW7

## Buttons
#Net "btns" LOC = B8 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L33P, Sch name = BTNS
#Net "btnu" LOC = A8 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L33N, Sch name = BTNU
#Net "btnl" LOC = C4 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L1N_VREF, Sch name = BTNL
#Net "btnd" LOC = C9 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L34N_GCLK18, Sch name = BTND
#Net "btnr" LOC = D9 | IOSTANDARD = LVCMOS33; # Bank = 0, pin name = IO_L34P_GCLK19, Sch name = BTNR

## VGA Connector
#NET "vgaRed<0> LOC = U7 | IOSTANDARD = LVCMOS33; # Bank = 2, pin name = IO_L43P, Sch name = RED0
#NET "vgaRed<1> LOC = V7 | IOSTANDARD = LVCMOS33; # Bank = 2, pin name = IO_L43N, Sch name = RED1
#NET vgaRed<2> LOC = N7 | IOSTANDARD = LVCMOS33; # Bank = 2, pin name = IO_L44P, Sch name = RED2
#NET vgaGreen<0> LOC = P8 | IOSTANDARD = LVCMOS33; # Bank = 2, pin name = IO_L44N, Sch name = GRN0
#NET vgaGreen<1> LOC = T6 | IOSTANDARD = LVCMOS33; # Bank = 2, pin name = IO_L45P, Sch name = GRN1
#NET vgaGreen<2> LOC = V6 | IOSTANDARD = LVCMOS33; # Bank = 2, pin name = IO_L45N, Sch name = GRN2
#NET vgaBlue<1> LOC = R7 | IOSTANDARD = LVCMOS33; # Bank = 2, pin name = IO_L46P, Sch name = BLU1
#NET vgaBlue<2> LOC = T7 | IOSTANDARD = LVCMOS33; # Bank = 2, pin name = IO_L46N, Sch name = BLU2

#NET "Hsync" LOC = N6 | IOSTANDARD = LVCMOS33; # Bank = 2, pin name = IO_L47P, Sch name = HSYNC
#NET "Vsync" LOC = P7 | IOSTANDARD = LVCMOS33; # Bank = 2, pin name = IO_L47N, Sch name = VSYNC

## 12 pin connectors

##JA
Net "JA<0>" LOC = T12 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L19P, Sch name = JA1
Net "JA<1>" LOC = V12 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L19N, Sch name = JA2  
Net "JA<2>" LOC = N10 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L20P, Sch name = JA3
Net "JA<3>" LOC = P11 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L20N, Sch name = JA4
Net "JA<4>" LOC = M10 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L22P, Sch name = JA7
Net "JA<5>" LOC = N9 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L22N, Sch name = JA8
Net "JA<6>" LOC = U11 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L23P, Sch name = JA9
Net "JA<7>" LOC = V11 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L23N, Sch name = JA10

#Initial columns to be high
#NET "JA<0>" PULLUP; 
#NET "JA<1>" PULLUP; 
#NET "JA<2>" PULLUP; 
#NET "JA<3>" PULLUP;

##JB
#Net "JB<0>" LOC = K2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L38P_M3DQ2, Sch name = JB1
#Net "JB<1>" LOC = K1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L38N_M3DQ3, Sch name = JB2
#Net "JB<2>" LOC = L4 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L39P_M3LDQS, Sch name = JB3
#Net "JB<3>" LOC = L3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L39N_M3LDQSN, Sch name = JB4
#Net "JB<4>" LOC = J3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L40P_M3DQ6, Sch name = JB7
#Net "JB<5>" LOC = J1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L40N_M3DQ7, Sch name = JB8
#Net "JB<6>" LOC = K3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L42N_GCLK24_M3LDM, Sch name = JB9
#Net "JB<7>" LOC = K5 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L43N_GCLK22_IRDY2_M3CASN, Sch name = JB10

##JC
#Net "JC<0>" LOC = H3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L44N_GCLK20_M3A6, Sch name = JC1
#Net "JC<1>" LOC = L7 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L45P_M3A3, Sch name = JC2
#Net "JC<2>" LOC = K6 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L45N_M3ODT, Sch name = JC3
#Net "JC<3>" LOC = G3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L46P_M3CLK, Sch name = JC4
#Net "JC<4>" LOC = G1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L46N_M3CLKN, Sch name = JC7
#Net "JC<5>" LOC = J7 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L47P_M3A0, Sch name = JC8
#Net "JC<6>" LOC = J6 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L47N_M3A1, Sch name = JC9
#Net "JC<7>" LOC = F2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L48P_M3BA0, Sch name = JC10

##JD, LX16 Die only
#Net "JD<0>" LOC = G11 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L40P, Sch name = JD1
#Net "JD<1>" LOC = F10 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L40N, Sch name = JD2
#Net "JD<2>" LOC = F11 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L42P, Sch name = JD3
#Net "JD<3>" LOC = E11 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L42N, Sch name = JD4
#Net "JD<4>" LOC = D12 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L47P, Sch name = JD7
#Net "JD<5>" LOC = C12 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L47N, Sch name = JD8
#Net "JD<6>" LOC = F12 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L51P, Sch name = JD9
#Net "JD<7>" LOC = E12 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L51N, Sch name = JD10

## VHDCI Connector
#Net "EXP-IO_P<0>" LOC = B2 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L2P, Sch name = EXP_IO1_P
#Net "EXP-IO_N<0>" LOC = A2 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L2N, Sch name = EXP_IO1_N
#Net "EXP-IO_P<1>" LOC = D6 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L3P, Sch name = EXP_IO2_P
#Net "EXP-IO_N<1>" LOC = C6 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L3N, Sch name = EXP_IO2_N
#Net "EXP-IO_P<2>" LOC = B3 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L4P, Sch name = EXP_IO3_P
#Net "EXP-IO_N<2>" LOC = A3 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L4N, Sch name = EXP_IO3_N
#Net "EXP-IO_P<3>" LOC = B4 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L5P, Sch name = EXP_IO4_P
#Net "EXP-IO_N<3>" LOC = A4 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L5N, Sch name = EXP_IO4_N
#Net "EXP-IO_P<4>" LOC = C5 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L6P, Sch name = EXP_IO5_P
#Net "EXP-IO_N<4>" LOC = A5 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L6N, Sch name = EXP_IO5_N
#Net "EXP-IO_P<5>" LOC = B6 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L8P, Sch name = EXP_IO6_P
#Net "EXP-IO_N<5>" LOC = A6 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L8N_VREF, Sch name = EXP_IO6_N
#Net "EXP-IO_P<6>" LOC = C7 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L10P, Sch name = EXP_IO7_P
#Net "EXP-IO_N<6>" LOC = A7 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L10N, Sch name = EXP_IO7_N
#Net "EXP-IO_P<7>" LOC = D8 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L11P, Sch name = EXP_IO8_P
#Net "EXP-IO_N<7>" LOC = C8 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L11N, Sch name = EXP_IO8_N
#Net "EXP-IO_P<8>" LOC = B9 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L35P_GCLK17, Sch name = EXP_IO9_P
#Net "EXP-IO_N<8>" LOC = A9 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L35N_GCLK16, Sch name = EXP_IO9_N
#Net "EXP-IO_P<9>" LOC = D11 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L36P_GCLK15, Sch name = EXP_IO10_P
#Net "EXP-IO_N<9>" LOC = C11 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L36N_GCLK14, Sch name = EXP_IO10_N
#Net "EXP-IO_P<10>" LOC = C10 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L37P_GCLK13, Sch name = EXP_IO11_P
#Net "EXP-IO_N<10>" LOC = A10 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L37N_GCLK12, Sch name = EXP_IO11_N
#Net "EXP-IO_P<11>" LOC = G9 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L38P, Sch name = EXP_IO12_P
#Net "EXP-IO_N<11>" LOC = F9 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L38N_VREF, Sch name = EXP_IO12_N
#Net "EXP-IO_P<12>" LOC = B11 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L39P, Sch name = EXP_IO13_P
#Net "EXP-IO_N<12>" LOC = A11 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L39N, Sch name = EXP_IO13_N
#Net "EXP-IO_P<13>" LOC = B12 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L41P, Sch name = EXP_IO14_P
#Net "EXP-IO_N<13>" LOC = A12 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L41N, Sch name = EXP_IO14_N
#Net "EXP-IO_P<14>" LOC = C13 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L50P, Sch name = EXP_IO15_P
#Net "EXP-IO_N<14>" LOC = A13 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L50N, Sch name = EXP_IO15_N
#Net "EXP-IO_P<15>" LOC = B14 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L62P, Sch name = EXP_IO16_P
#Net "EXP-IO_N<15>" LOC = A14 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L62N_VREF, Sch name = EXP_IO16_N
#Net "EXP-IO_P<16>" LOC = F13 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L63P_SCP7, Sch name = EXP_IO17_P
#Net "EXP-IO_N<16>" LOC = E13 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L63N_SCP6, Sch name = EXP_IO17_N
#Net "EXP-IO_P<17>" LOC = C15 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L64P_SCP5, Sch name = EXP_IO18_P
#Net "EXP-IO_N<17>" LOC = A15 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L64N_SCP4, Sch name = EXP_IO18_N
#Net "EXP-IO_P<18>" LOC = D14 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L65P_SCP3, Sch name = EXP_IO19_P
#Net "EXP-IO_N<18>" LOC = C14 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L65N_SCP2, Sch name = EXP_IO19_N
#Net "EXP-IO_P<19>" LOC = B16 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L66P_SCP1, Sch name = EXP_IO20_P
#Net "EXP-IO_N<19>" LOC = A16 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L66N_SCP0, Sch name = EXP_IO20_N
