Par Statistics
Total Non-vccgnd Signals=813
Total Non-vccgnd Design Pins=3501
Total Non-vccgnd Conns=3501
Total Non-vccgnd Timing Constrained Conns=3412
Phase 1 CPU=4.6 sec
Phase 2 CPU=4.9 sec
Phase 3 CPU=6.0 sec
Phase 4 CPU=6.9 sec
Phase 5 CPU=8.7 sec
Phase 6 CPU=8.7 sec
Phase 7 CPU=8.7 sec
Phase 8 CPU=8.7 sec
Phase 9 CPU=8.7 sec
Phase 10 CPU=8.9 sec
AvgWirelenPerPin Fanout 1=1.0
AvgWirelenPerPin Fanout 2=2.0
AvgWirelenPerPin Fanout 3=1.7
AvgWirelenPerPin Fanout 4=2.5
AvgWirelenPerPin Fanout 10=2.8
AvgWirelenPerPin Fanout 50=2.4
AvgWirelenPerPin Fanout 100=4.6
AvgWirelenPerPin Fanout 500=5.3
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.7402