Net "CLK" LOC=V10 | IOSTANDARD=LVCMOS33;
Net "CLK" TNM_NET = sys_clk_pin;
TIMESPEC TS_sys_clk_pin = PERIOD sys_clk_pin 100000 kHz;

##JA
Net "CS" LOC = T12 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L19P, Sch name = JA1
Net "SDIN" LOC = V12 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L19N, Sch name = JA2  
Net "SCLK" LOC = P11 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L20N, Sch name = JA4
Net "DC" LOC = M10 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L22P, Sch name = JA7
Net "RES" LOC = N9 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L22N, Sch name = JA8
Net "VBAT" LOC = U11 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L23P, Sch name = JA9
Net "VDD" LOC = V11 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L23N, Sch name = JA10

##Buttons
Net "RST" LOC = B8 | IOSTANDARD = LVCMOS33; #Bank = 0, pin name = IO_L33P, Sch name = BTNS

## Switches
Net "finished" LOC = T10 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L29N_GCLK2, Sch name = SW0

##JC
Net "COLo<0>" LOC = H3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L44N_GCLK20_M3A6, Sch name = JC1
Net "COLo<1>" LOC = L7 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L45P_M3A3, Sch name = JC2
Net "COLo<2>" LOC = K6 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L45N_M3ODT, Sch name = JC3
Net "COLo<3>" LOC = G3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L46P_M3CLK, Sch name = JC4
Net "ROWi<0>" LOC = G1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L46N_M3CLKN, Sch name = JC7
Net "ROWi<1>" LOC = J7 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L47P_M3A0, Sch name = JC8
Net "ROWi<2>" LOC = J6 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L47N_M3A1, Sch name = JC9
Net "ROWi<3>" LOC = F2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L48P_M3BA0, Sch name = JC10