Par Statistics
Total Non-vccgnd Signals=183
Total Non-vccgnd Design Pins=592
Total Non-vccgnd Conns=592
Total Non-vccgnd Timing Constrained Conns=486
Phase 1 CPU=3.9 sec
Phase 2 CPU=4.2 sec
Phase 3 CPU=4.4 sec
Phase 4 CPU=5.0 sec
Phase 5 CPU=5.3 sec
Phase 6 CPU=5.3 sec
Phase 7 CPU=5.3 sec
Phase 8 CPU=5.3 sec
Phase 9 CPU=5.3 sec
Phase 10 CPU=5.3 sec
AvgWirelenPerPin Fanout 1=2.0
AvgWirelenPerPin Fanout 2=1.5
AvgWirelenPerPin Fanout 3=6.3
AvgWirelenPerPin Fanout 4=3.3
AvgWirelenPerPin Fanout 10=3.5
AvgWirelenPerPin Fanout 50=2.8
AvgWirelenPerPin Fanout 100=0.0
AvgWirelenPerPin Fanout 500=0.0
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.0385