<?xml version="1.0" encoding="UTF-8"?>
<!-- IMPORTANT: This is an internal file that has been generated
     by the Xilinx ISE software.  Any direct editing or
     changes made to this file may result in unpredictable
     behavior or data corruption.  It is strongly advised that
     users do not edit the contents of this file. -->
<messages>
<msg type="warning" file="UtilitiesC" num="159" delta="old" >Message file &quot;<arg fmt="%s" index="1">usenglish/ip.msg</arg>&quot; wasn&apos;t found.
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">0</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">9</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%d" index="1">0</arg>: (<arg fmt="%d" index="2">0</arg>,<arg fmt="%d" index="3">0</arg>) 	: <arg fmt="%d" index="4">9</arg>x<arg fmt="%d" index="5">2048</arg> 	u:<arg fmt="%d" index="6">8</arg>
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_input_block.vhd" Line 691: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_input_block.vhd" Line 707: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="warning" file="HDLCompiler" num="746" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_prim_width.vhd" Line 977: Range is empty (null range)
</msg>

<msg type="warning" file="HDLCompiler" num="220" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_prim_width.vhd" Line 977: Assignment ignored
</msg>

<msg type="warning" file="HDLCompiler" num="746" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_prim_width.vhd" Line 978: Range is empty (null range)
</msg>

<msg type="warning" file="HDLCompiler" num="220" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_prim_width.vhd" Line 978: Assignment ignored
</msg>

<msg type="info" file="ip" num="0" delta="new" >Reading MIF file at <arg fmt="%s" index="1">C:/Users/URBicz/Desktop/PmodOLED_graphic_v2/ipcore_dir/tmp/_cg/charLib.mif</arg>
</msg>

<msg type="warning" file="ip" num="0" delta="new" >Memory initialization file (<arg fmt="%s" index="1">charLib.mif</arg>) depth is smaller than memory depth.
</msg>

<msg type="warning" file="ip" num="0" delta="new" >Memory initialization file (<arg fmt="%s" index="1">charLib.mif</arg>) has words wider than <arg fmt="%0d" index="2">8</arg> bits, right-aligning.
</msg>

<msg type="info" file="ip" num="0" delta="new" >Default data (<arg fmt="%s" index="1">0</arg> hex) will persist where not overwritten by MIF file.
</msg>

<msg type="info" file="ip" num="0" delta="new" ><arg fmt="%s" index="1">$Id: get_init_bmg_v6_2.c,v 1.1 2011/02/07 06:43:48 muruga Exp $</arg>
</msg>

<msg type="info" file="ip" num="0" delta="new" >Reading MIF file at <arg fmt="%s" index="1">C:/Users/URBicz/Desktop/PmodOLED_graphic_v2/ipcore_dir/tmp/_cg/charLib.mif</arg>
</msg>

<msg type="warning" file="ip" num="0" delta="new" >Memory initialization file (<arg fmt="%s" index="1">charLib.mif</arg>) depth is smaller than memory depth.
</msg>

<msg type="warning" file="ip" num="0" delta="new" >Memory initialization file (<arg fmt="%s" index="1">charLib.mif</arg>) has words wider than <arg fmt="%0d" index="2">8</arg> bits, right-aligning.
</msg>

<msg type="info" file="ip" num="0" delta="new" >Default data (<arg fmt="%s" index="1">0</arg> hex) will persist where not overwritten by MIF file.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_prim_wrapper_s6_init.vhd" Line 493: Net &lt;<arg fmt="%s" index="1">pad_addr_b14[13]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_prim_wrapper_s6_init.vhd" Line 502: Net &lt;<arg fmt="%s" index="1">pad_din_b32[31]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_prim_wrapper_s6_init.vhd" Line 505: Net &lt;<arg fmt="%s" index="1">pad_dinp_b4[3]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_prim_wrapper_s6_init.vhd" Line 531: Net &lt;<arg fmt="%s" index="1">doutb_i[8]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_prim_width.vhd" Line 429: Net &lt;<arg fmt="%s" index="1">dina_pad[8]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="634" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_prim_width.vhd" Line 433: Net &lt;<arg fmt="%s" index="1">dinb_pad[8]</arg>&gt; does not have a driver.
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_generic_cstr.vhd" Line 1544: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="warning" file="HDLCompiler" num="321" delta="old" >"C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_generic_cstr.vhd" Line 1557: Comparison between arrays of unequal length always returns <arg fmt="%s" index="1">FALSE</arg>.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">doutb</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">rdaddrecc</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_bid</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_bresp</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rid</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rdata</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rresp</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rdaddrecc</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">sbiterr</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">dbiterr</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_awready</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_wready</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_bvalid</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_arready</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rlast</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_rvalid</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_sbiterr</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\charLib.vhd</arg>&quot; line <arg fmt="%s" index="2">148</arg>: Output port &lt;<arg fmt="%s" index="3">s_axi_dbiterr</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">U0</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWID</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWADDR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWLEN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWSIZE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWBURST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_WDATA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_WSTRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARID</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARADDR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARLEN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARSIZE</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARBURST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AClk</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_ARESETN</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_AWVALID</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_WLAST</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_WVALID</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_BREADY</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_ARVALID</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_RREADY</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">S_AXI_INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="2935" delta="old" >Signal &apos;<arg fmt="%s" index="1">S_AXI_BID</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_v6_2_xst</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_BRESP</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="old" >Signal &apos;<arg fmt="%s" index="1">S_AXI_RID</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_v6_2_xst</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_RDATA</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_RRESP</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_RDADDRECC</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_AWREADY</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_WREADY</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_BVALID</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_ARREADY</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_RLAST</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_RVALID</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">S_AXI_DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">WEA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">DINA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">WEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">RSTA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">ENA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">CLKB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">RSTB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">INJECTDBITERR_I</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">INJECTSBITERR_I</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEA</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1341</arg>: Output port &lt;<arg fmt="%s" index="3">SBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[0].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="info" file="Xst" num="3210" delta="old" >&quot;<arg fmt="%s" index="1">C:\Users\URBicz\Desktop\PmodOLED_graphic_v2\ipcore_dir\tmp\_cg\_dbg\blk_mem_gen_v6_2\blk_mem_gen_generic_cstr.vhd</arg>&quot; line <arg fmt="%s" index="2">1341</arg>: Output port &lt;<arg fmt="%s" index="3">DBITERR</arg>&gt; of the instance &lt;<arg fmt="%s" index="4">ramloop[0].ram.r</arg>&gt; is unconnected or connected to loadless signal.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">RDADDRECC</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTSBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">INJECTDBITERR</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="2935" delta="old" >Signal &apos;<arg fmt="%s" index="1">dina_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="old" >Signal &apos;<arg fmt="%s" index="1">dinb_pad&lt;8&gt;</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_width</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0</arg>).
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">WEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">ADDRB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">DINB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">ENB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">REGCEB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">pad_addr_b14</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="2935" delta="old" >Signal &apos;<arg fmt="%s" index="1">pad_din_b32</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_init</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">00000000000000000000000000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="old" >Signal &apos;<arg fmt="%s" index="1">pad_dinp_b4</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_init</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">0000</arg>).
</msg>

<msg type="warning" file="Xst" num="2935" delta="old" >Signal &apos;<arg fmt="%s" index="1">doutb_i</arg>&apos;, unconnected in block &apos;<arg fmt="%s" index="2">blk_mem_gen_prim_wrapper_s6_init</arg>&apos;, is tied to its initial value (<arg fmt="%s" index="3">000000000</arg>).
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">DOUTB_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">RDADDRECC_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">CLKB</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">SBITERR_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="647" delta="old" >Input &lt;<arg fmt="%s" index="1">DBITERR_I</arg>&gt; is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">RDADDRECC</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">SBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="warning" file="Xst" num="653" delta="old" >Signal &lt;<arg fmt="%s" index="1">DBITERR</arg>&gt; is used but never assigned. This sourceless signal will be automatically connected to value <arg fmt="%s" index="2">GND</arg>.
</msg>

<msg type="info" file="Xst" num="2169" delta="old" >HDL ADVISOR - Some clock signals were not automatically buffered by XST with BUFG/BUFR resources. Please use the buffer_type constraint in order to insert these buffers to the clock signals to help prevent skew problems.
</msg>

</messages>

