Creating log file
C:\Users\URBicz\Desktop\diplomka\Pmod\PmodOLEDctrl\PmodOLED_Source\PmodOLEDCtrl_
xpa.log.
Loading device for application Rf_Device from file '6slx16.nph' in environment
C:\Xilinx\14.3\ISE_DS\ISE\.
   "PmodOLEDCtrl" is an NCD, version 3.2, device xc6slx16, package csg324, speed
-3

INFO:Power:1693 - 
   --------------------------------------------------------------
                         The power estimate will be calculated using PRODUCTION
   data.
   --------------------------------------------------------------

Design load 20% complete
Design load 25% complete
Design load 30% complete
Design load 60% complete
Design load 95% complete
Design load 100% complete
Running Vector-less Activity Propagation
..............
Finished Running Vector-less Activity Propagation
Finished Running Vector-less Activity Propagation 0 secs 

Design 'PmodOLEDCtrl.ncd' and constraints 'PmodOLEDCtrl.pcf' opened successfully

