Par Statistics
Total Non-vccgnd Signals=808
Total Non-vccgnd Design Pins=3474
Total Non-vccgnd Conns=3474
Total Non-vccgnd Timing Constrained Conns=3385
Phase 1 CPU=4.1 sec
Phase 2 CPU=4.4 sec
Phase 3 CPU=5.4 sec
Phase 4 CPU=6.0 sec
Phase 5 CPU=7.2 sec
Phase 6 CPU=7.2 sec
Phase 7 CPU=7.2 sec
Phase 8 CPU=7.2 sec
Phase 9 CPU=7.2 sec
Phase 10 CPU=7.3 sec
AvgWirelenPerPin Fanout 1=2.0
AvgWirelenPerPin Fanout 2=2.0
AvgWirelenPerPin Fanout 3=1.7
AvgWirelenPerPin Fanout 4=2.8
AvgWirelenPerPin Fanout 10=3.5
AvgWirelenPerPin Fanout 50=3.3
AvgWirelenPerPin Fanout 100=6.8
AvgWirelenPerPin Fanout 500=5.4
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.5493