Creating log file
C:\Users\URBicz\Desktop\diplomka\final\prilohy\uloha2\reseni\OLED_ctrl_V1_0_shif
ting\OLED_ctrl_xpa.log.
Loading device for application Rf_Device from file '6slx16.nph' in environment
C:\Xilinx\14.3\ISE_DS\ISE\.
   "OLED_ctrl" is an NCD, version 3.2, device xc6slx16, package csg324, speed -3

INFO:Power:1693 - 
   --------------------------------------------------------------
                         The power estimate will be calculated using PRODUCTION
   data.
   --------------------------------------------------------------

Design load 20% complete
Design load 25% complete
Design load 30% complete
Design load 60% complete
Design load 95% complete
Design load 100% complete
Running Vector-less Activity Propagation
........
Finished Running Vector-less Activity Propagation
Finished Running Vector-less Activity Propagation 0 secs 

Design 'OLED_ctrl.ncd' and constraints 'OLED_ctrl.pcf' opened successfully

