Par Statistics
Total Non-vccgnd Signals=1393
Total Non-vccgnd Design Pins=3747
Total Non-vccgnd Conns=3747
Total Non-vccgnd Timing Constrained Conns=3680
Phase 1 CPU=4.4 sec
Phase 2 CPU=4.7 sec
Phase 3 CPU=6.5 sec
Phase 4 CPU=7.3 sec
Phase 5 CPU=10.3 sec
Phase 6 CPU=10.3 sec
Phase 7 CPU=10.3 sec
Phase 8 CPU=10.3 sec
Phase 9 CPU=10.3 sec
Phase 10 CPU=10.7 sec
AvgWirelenPerPin Fanout 1=2.0
AvgWirelenPerPin Fanout 2=2.5
AvgWirelenPerPin Fanout 3=1.7
AvgWirelenPerPin Fanout 4=2.8
AvgWirelenPerPin Fanout 10=2.3
AvgWirelenPerPin Fanout 50=3.6
AvgWirelenPerPin Fanout 100=13.9
AvgWirelenPerPin Fanout 500=6.3
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.9177