
## Clock signal
Net "clk" LOC=V10 | IOSTANDARD=LVCMOS33;
Net "clk" TNM_NET = sys_clk_pin;
TIMESPEC TS_sys_clk_pin = PERIOD sys_clk_pin 100000 kHz;

## JA
Net "OLED_CS" LOC = T12 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L19P, Sch name = JA1
Net "OLED_MOSI" LOC = V12 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L19N, Sch name = JA2  
Net "OLED_SCLK" LOC = P11 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L20N, Sch name = JA4
Net "OLED_D_nC" LOC = M10 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L22P, Sch name = JA7
Net "OLED_RES" LOC = N9 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L22N, Sch name = JA8
Net "OLED_VBATC" LOC = U11 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L23P, Sch name = JA9
Net "OLED_VDDC" LOC = V11 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L23N, Sch name = JA10

## Switches
#Net "col<0>" LOC = T10 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L29N_GCLK2, Sch name = SW0
#Net "col<1>" LOC = T9 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L32P_GCLK29, Sch name = SW1
#Net "col<2>" LOC = V9 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L32N_GCLK28, Sch name = SW2
#Net "col<3>" LOC = M8 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L40P, Sch name = SW3
#Net "line<0>" LOC = N8 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L40N, Sch name = SW4
#Net "line<1>" LOC = U8 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L41P, Sch name = SW5
#Net "char_write" LOC = V8 | IOSTANDARD = LVCMOS33; #Bank = 2, pin name = IO_L41N_VREF, Sch name = SW6
Net "resetn" LOC = T5 | IOSTANDARD = LVCMOS33; #Bank = MISC, pin name = IO_L48N_RDWR_B_VREF_2, Sch name = SW7

## JC
Net "JC<0>" LOC = H3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L44N_GCLK20_M3A6, Sch name = JC1
Net "JC<1>" LOC = L7 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L45P_M3A3, Sch name = JC2
Net "JC<2>" LOC = K6 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L45N_M3ODT, Sch name = JC3
Net "JC<3>" LOC = G3 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L46P_M3CLK, Sch name = JC4
Net "JC<4>" LOC = G1 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L46N_M3CLKN, Sch name = JC7
Net "JC<5>" LOC = J7 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L47P_M3A0, Sch name = JC8
Net "JC<6>" LOC = J6 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L47N_M3A1, Sch name = JC9
Net "JC<7>" LOC = F2 | IOSTANDARD = LVCMOS33; #Bank = 3, pin name = IO_L48P_M3BA0, Sch name = JC10