Par Statistics
Total Non-vccgnd Signals=1195
Total Non-vccgnd Design Pins=3381
Total Non-vccgnd Conns=3381
Total Non-vccgnd Timing Constrained Conns=3314
Phase 1 CPU=4.4 sec
Phase 2 CPU=4.8 sec
Phase 3 CPU=6.2 sec
Phase 4 CPU=6.8 sec
Phase 5 CPU=8.7 sec
Phase 6 CPU=8.7 sec
Phase 7 CPU=8.7 sec
Phase 8 CPU=8.7 sec
Phase 9 CPU=8.7 sec
Phase 10 CPU=8.9 sec
AvgWirelenPerPin Fanout 1=2.0
AvgWirelenPerPin Fanout 2=1.5
AvgWirelenPerPin Fanout 3=1.0
AvgWirelenPerPin Fanout 4=1.8
AvgWirelenPerPin Fanout 10=1.9
AvgWirelenPerPin Fanout 50=3.4
AvgWirelenPerPin Fanout 100=6.3
AvgWirelenPerPin Fanout 500=4.1
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.7003