Release 14.3 - ngc2edif P.40xd (nt)
Copyright (c) 1995-2012 Xilinx, Inc.  All rights reserved.
Reading design OLED_ctrl.ngc ...
WARNING:NetListWriters:298 - No output is written to OLED_ctrl.xncf, ignored.
Processing design ...
   Preping design's networks ...
   Preping design's macros ...
WARNING:NetListWriters:306 - Signal bus
   CPU/Msub_GND_7_o_GND_7_o_sub_217_OUT<7:0>_cy<4 : 2> on block OLED_ctrl is not
   reconstructed, because there are some missing bus signals.
WARNING:NetListWriters:306 - Signal bus
   CPU/Madd_local_data[7]_GND_7_o_add_222_OUT_cy<5 : 3> on block OLED_ctrl is
   not reconstructed, because there are some missing bus signals.
  finished :Prep
Writing EDIF netlist file OLED_ctrl.edif ...
ngc2edif: Total memory usage is 80504 kilobytes

