Building configuration...

Current configuration : 11080 bytes
!
! Last configuration change at 18:20:42 UTC Fri May 20 2022 by tzboril
!
version 17.4
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname R3
!
boot-start-marker
boot-end-marker
!
!
!
aaa new-model
!
!
aaa authentication login default local
aaa authorization exec default local
!
!
!
!
!
!
aaa session-id common
!
!
!
!
!
!
!
no ip domain lookup
ip domain name xzbori22.vutbr.cz
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
!
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-3820994395
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-3820994395
 revocation-check none
 rsakeypair TP-self-signed-3820994395
!
crypto pki trustpoint SLA-TrustPoint
 enrollment terminal
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-668508874
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-668508874
 revocation-check none
 rsakeypair TP-self-signed-668508874
!
!
crypto pki certificate chain TP-self-signed-3820994395
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 33383230 39393433 3935301E 170D3232 30323037 31383130
  35395A17 0D333230 32303731 38313035 395A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D33 38323039
  39343339 35308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100E2F1 8566A32B A22259A3 4E760170 74B35644 66C82D3D 032A11A0
  804A425C 64FB6C16 93883E5B E6E7E8D1 2E2C2F6B E45BF090 5C387179 41A68899
  598F59AF D5660EEF ACF3C612 7D581468 78DECDE7 1B54ADE1 B29CE2E0 FCCC658A
  2EE08E6F DE85C643 2518FD0C 1A0A472C 2EDAE36A 456A2EF4 2BF2E307 F45E4DCE
  C116DE31 66389967 023F3672 07B3D31D 3DD5E532 6524FBB6 D8B1CA94 3B854ADB
  72C465AE C0E1BEF1 0398E5F0 2EAAE1DA 4B0E45C6 0C1D3B39 6FCB7166 FB487723
  ADE57C11 9857C589 1DF4351F A3B30DEA 86F5E1CF DA57B50F 7BD7EFCA DF321829
  0D1A53A2 F3F165C7 369476A6 2287A67A 7F8CA846 298B8636 9B4C105B 169BB2DA
  3245FD77 64410203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 14BB6459 0D9AB452 E1FBB52A CAE79C71 87BBA66F
  98301D06 03551D0E 04160414 BB64590D 9AB452E1 FBB52ACA E79C7187 BBA66F98
  300D0609 2A864886 F70D0101 05050003 82010100 25441E67 FA8CB790 41DBE726
  B76FA8F3 CDFA7664 BD54BA97 7ADFC088 ED9CF0D3 7CC08846 182F36C1 EF60A3CC
  DCE1218F AE941257 2EFAE987 96E1D9B5 3A553BE5 8B16B516 B0FCAAA4 536E999A
  6F35A892 06CAB2E0 5F4D0D3A 29E1BE51 6444C85B 369AE39C 1B5AA503 B9E70734
  BAE3DBA1 A6EFC2B0 15589589 3E7F811E 4C2F2BC0 38929122 996FE9C3 6CFE3530
  9ABA622C D68DE587 ACC3B762 A2C2555D E913B150 9824B9E1 778FA5E6 4FC378ED
  2F761F44 DDFCFBDA B664BBDD 09785FF0 4D73E9D3 E646D750 58D68697 FC6425E2
  7812BBB8 491D298D BD51DA2A D5E10EF8 831A5231 D0F0BFB9 4FD5A302 CD27E073
  F28E4385 28FAEF3E 605C1A6C 86B92DDD 5A34969D
  	quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
  	quit
crypto pki certificate chain TP-self-signed-668508874
!
license udi pid C8000V sn 97M4BMKXHQR
diagnostic bootup level minimal
memory free low-watermark processor 69173
!
!
username tzboril privilege 15 secret 9 $9$vmjg1Guf9zAs2E$.9eGTyCDIMm1xuPs6T5H0yTTXKmmZX9schGiQeY4xVM
!
redundancy
!
!
!
cdp run
!
!
!
!
!
!
interface GigabitEthernet1
 description To Router2
 ip address 192.168.1.2 255.255.255.252
 ip ospf authentication-key cisco
 negotiation auto
 cdp enable
!
interface GigabitEthernet2
 description To Router4
 ip address 192.168.2.1 255.255.255.252
 negotiation auto
 cdp enable
!
interface GigabitEthernet3
 description To R1_bypass
 ip address 192.168.123.2 255.255.255.252
 ip ospf authentication-key cisco
 negotiation auto
 cdp enable
!
interface GigabitEthernet4
 ip address 10.255.255.3 255.255.255.0
 negotiation auto
!
router ospf 109
 area 0 authentication
 passive-interface GigabitEthernet1
 passive-interface GigabitEthernet2
 network 10.0.0.2 0.0.0.0 area 2
 network 192.168.1.2 0.0.0.0 area 0
 network 192.168.2.1 0.0.0.0 area 2
 network 192.168.123.2 0.0.0.0 area 0
!
router bgp 200
 bgp log-neighbor-changes
 no bgp default ipv4-unicast
 neighbor 192.168.2.2 remote-as 100
 !
 address-family ipv4
  redistribute ospf 109
  neighbor 192.168.2.2 activate
 exit-address-family
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
ip route 192.168.122.0 255.255.255.0 GigabitEthernet3
ip ssh version 2
ip scp server enable
!
!
!
snmp-server group group_1 v3 priv
snmp-server community cisco RO
snmp-server enable traps snmp authentication linkdown linkup coldstart warmstart
snmp-server enable traps vrrp
snmp-server enable traps pfr
snmp-server enable traps flowmon
snmp-server enable traps ds1
snmp-server enable traps entity-perf throughput-notif
snmp-server enable traps call-home message-send-fail server-fail
snmp-server enable traps tty
snmp-server enable traps casa
snmp-server enable traps ospf state-change
snmp-server enable traps ospf errors
snmp-server enable traps ospf retransmit
snmp-server enable traps ospf lsa
snmp-server enable traps ospf cisco-specific state-change nssa-trans-change
snmp-server enable traps ospf cisco-specific state-change shamlink interface
snmp-server enable traps ospf cisco-specific state-change shamlink neighbor
snmp-server enable traps ospf cisco-specific errors
snmp-server enable traps ospf cisco-specific retransmit
snmp-server enable traps ospf cisco-specific lsa
snmp-server enable traps eigrp
snmp-server enable traps adslline
snmp-server enable traps vdsl2line
snmp-server enable traps license
snmp-server enable traps smart-license
snmp-server enable traps ethernet evc status create delete
snmp-server enable traps ether-oam
snmp-server enable traps ethernet cfm cc mep-up mep-down cross-connect loop config
snmp-server enable traps ethernet cfm crosscheck mep-missing mep-unknown service-up
snmp-server enable traps entity-qfp mem-res-thresh throughput-notif
snmp-server enable traps entity-state
snmp-server enable traps diameter
snmp-server enable traps vtp
snmp-server enable traps vlancreate
snmp-server enable traps vlandelete
snmp-server enable traps port-security
snmp-server enable traps c3g
snmp-server enable traps LTE
snmp-server enable traps isdn call-information
snmp-server enable traps isdn layer2
snmp-server enable traps isdn chan-not-avail
snmp-server enable traps isdn ietf
snmp-server enable traps bgp cbgp2
snmp-server enable traps dlsw
snmp-server enable traps entity-sensor
snmp-server enable traps resource-policy
snmp-server enable traps flash insertion removal lowspace
snmp-server enable traps nhrp nhs
snmp-server enable traps nhrp nhc
snmp-server enable traps nhrp nhp
snmp-server enable traps nhrp quota-exceeded
snmp-server enable traps ipsla
snmp-server enable traps cnpd
snmp-server enable traps entity-diag boot-up-fail hm-test-recover hm-thresh-reached scheduled-test-fail
snmp-server enable traps auth-framework sec-violation
snmp-server enable traps bfd
snmp-server enable traps cef resource-failure peer-state-change peer-fib-state-change inconsistency
snmp-server enable traps memory bufferpeak
snmp-server enable traps config-copy
snmp-server enable traps config
snmp-server enable traps config-ctid
snmp-server enable traps dhcp
snmp-server enable traps fru-ctrl
snmp-server enable traps entity
snmp-server enable traps event-manager
snmp-server enable traps frame-relay
snmp-server enable traps frame-relay subif
snmp-server enable traps hsrp
snmp-server enable traps pimstdmib neighbor-loss invalid-register invalid-join-prune rp-mapping-change interface-election
snmp-server enable traps ipmulticast
snmp-server enable traps isis
snmp-server enable traps ip local pool
snmp-server enable traps msdp
snmp-server enable traps mvpn
snmp-server enable traps ospfv3 state-change
snmp-server enable traps ospfv3 errors
snmp-server enable traps pim neighbor-change rp-mapping-change invalid-pim-message
snmp-server enable traps pppoe
snmp-server enable traps cpu threshold
snmp-server enable traps rsvp
snmp-server enable traps l2tun session
snmp-server enable traps l2tun pseudowire status
snmp-server enable traps aaa_server
snmp-server enable traps atm subif
snmp-server enable traps pki
snmp-server enable traps ethernet cfm alarm
snmp-server enable traps alarms informational
snmp-server enable traps rf
snmp-server enable traps transceiver all
snmp-server enable traps bulkstat collection transfer
snmp-server enable traps vrfmib vrf-up vrf-down vnet-trunk-up vnet-trunk-down
!
!
!
!
control-plane
!
!
line con 0
 stopbits 1
line aux 0
line vty 0 4
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
!
end