EXFO Electro-Optical Engineering Inc.
Report Title: r
Report Date: 1/4/2000 22:10:54
--------------------------------Job Information--------------------------------
Job ID:          1078356
Contractor:                                  
Customer:        Melo
Operator Name:   Kloudný
Comment:         měření propoje Uherské Hradiště --- Zlín (300Mbps)

--------------------------------Test Configuration--------------------------------
Test Name:          TEST                   
Interface Type:     Ethernet 10/100/1000   
Application Type:   RFC 2544               
Topology:           Single Port            

>Port Configuration
                     Port 1              
Transceiver Mode     Electrical          
Speed                100Mbps               
Duplex mode          Full                
Auto-Negotiation     Disabled            
VLAN                 None                
IP Source Address    192.168.1.5       
MAC Source Address   00:03:01:FC:73:56    

>RFC 2544
Local to Remote Throughput Maximum Rate (%)   100     
Remote to Local Throughput Maximum Rate (%)   100     
Throughput Test Time                          00:01   
Back-to-Back Test Time                        00:02   
Local to Remote Frame Loss Maximum Rate (%)   100     
Remote to Local Frame Loss Maximum Rate (%)   100     
Frame Loss Test Time                          00:01   
Latency Test Time                            00:01   
Margin (%)                            0       

Latency Max rate
No information is available

>Remote Dual Test Set
No information is available

--------------------------------Test Results--------------------------------
Start Time:    2010-02-19 03:01:42   Duration   0d 00:03:25

>RFC 2544
Verdict        Status   
Throughput     Completed
Back-to-Back   Completed
Frame Loss     Completed
Latency        Completed

>Throughput
Layer: All Layer
Display Results: Current
Frame Size   Local to Remote (Mbps)   Remote to Local (Mbps)   
64           100                      100                     
128          100                      100                     
256          100                      100                     
512          100                      100                     
1024         100                      100                       
1280         100                      100                       
1518         100                      100

>Back-to-Back
Layer: All Layer
Display Results: Current
Frame Size   Local to Remote (Frames/Burst)   Remote to Local (Frames/Burst)   
64           1488096                          1488096                          
128          844595                           844595                           
256          --                            --                            
512          --                            --                            
1024         --                            --                            
1280         --                            --                            
1518         --                            --                            

>Frame Loss
Display Results: Current
Displayed Step: --
Frame Size   Local to Remote(%)   Remote to Local(%)   
64           0.0                  0.0                   
128          0.0                  0.0                   
256          0.0                  0.0                   
512          0.0                  0.0                   
1024         0.0                  0.0                   
1280         0.0                  0.0                   
1518         0.0                  0.0                   

>Latency
Display Results: Current
Latency Mode: Cut Through
Frame Size   Round Trip Time (ms)   
64           0.04542                     
128          0.04501                     
256          0.04527                     
512          0.04511                     
1024         0.04527                     
1280         0.04532                     
1518         0.04537

--------------------------------Alarms/Errors--------------------------------
>Port
Alarms
            Seconds   
Frequency   0        

>Ethernet
Alarms
       Seconds   
Link   0         

Errors
                Seconds   Count   Rate       
Symbol          0         0       0,00E00    
Idle            1         255     3,69E-07   
False Carrier   1         4607    1,05E-02   
FCS             0         0       0,00E00    
Jabber/Giant    0         0       0,00E00    
Runt            0         0       0,00E00    
Undersize       0         0       0,00E00    
Alignment       --        --      --         

>Upper Layer
Errors
                     Seconds   Count   Rate      
IP Header Checksum   0         0       0,00E00   
UDP Checksum         0         0       0,00E00   

--------------------------------Statistics--------------------------------
Valid Frame Counts
Total TX Frame Count   3324806
Total RX Frame Count   3325845

Frequency Analysis
Frequency (bps)              --    
Frequency Offset (ppm)       0
Max. Negative Offset (ppm)   0
Max. Positive Offset (ppm)   0

--------------------------------System Information--------------------------------
>Module Information
Module ID:          AXS-855  
Revision:           65       
Serial Number:      517757   
Calibration Date:   1/1/1970 

>Software Information
Software Version:   1.3.1.31 

