EXFO Electro-Optical Engineering Inc.
Report Title: ReportTitle
Report Date: 2010-02-19 03:07:30
--------------------------------Job Information--------------------------------
Job ID:          1                            
Contractor:                                  
Customer:        Maxprogres                            
Operator Name:   Zdenek                            
Comment:         mereni propoje Boskovice --- PVT (300Mbps)   Pozn. mereno bez aktivnich prvku, switche, routery apod.   

--------------------------------Test Configuration--------------------------------
Test Name:          TEST                   
Interface Type:     Ethernet 10/100/1000   
Application Type:   RFC 2544               
Topology:           Single Port            

>Port Configuration
                     Port 1              
Transceiver Mode     Electrical          
Speed                1Gbps               
Duplex mode          Full                
Auto-Negotiation     Disabled            
VLAN                 None                
IP Source Address    192.168.1.100       
MAC Source Address   00:03:01:08:3A:AD   

>RFC 2544
Local to Remote Throughput Maximum Rate (%)   30      
Remote to Local Throughput Maximum Rate (%)   30      
Throughput Test Time                          00:01   
Back-to-Back Test Time                        00:01   
Local to Remote Frame Loss Maximum Rate (%)   100     
Remote to Local Frame Loss Maximum Rate (%)   100     
Frame Loss Test Time                          00:01   
Latency Test Time                            00:01   
Margin (%)                            0       

Latency Max rate
No information is available

>Remote Dual Test Set
No information is available

--------------------------------Test Results--------------------------------
Start Time:    2010-02-19 03:01:42   Duration   0d 00:03:25   

>RFC 2544
Verdict        Status   
Throughput     --       
Back-to-Back   --       
Frame Loss     --       
Latency        --       

>Throughput
Layer: Layer 1-2-3
Display Results: Current
Frame Size   Local to Remote (Mbps)   Remote to Local (Mbps)   
64           299,999467               300                      
128          300,20284                300,20284                
256          299,999467               299,999148               
512          300,056402               300,055549               
1024         299,999467               300                      
1280         300,023079               300,022227               
1518         299,980495               299,980495               

>Back-to-Back
Layer: Layer 1-2-3
Display Results: Current
Frame Size   Local to Remote (Frames/Burst)   Remote to Local (Frames/Burst)   
64           1488096                          1488096                          
128          844595                           844595                           
256          --                            --                            
512          --                            --                            
1024         --                            --                            
1280         --                            --                            
1518         --                            --                            

>Frame Loss
Display Results: Current
Displayed Step: 100
Frame Size   Local to Remote(%)   Remote to Local(%)   
64           --                   --                   
128          --                   --                   
256          --                   --                   
512          --                   --                   
1024         --                   --                   
1280         --                   --                   
1518         --                   --                   

>Latency
Display Results: Current
Latency Mode: Cut Through
Frame Size   Round Trip Time (ms)   
64           --                     
128          --                     
256          --                     
512          --                     
1024         --                     
1280         --                     
1518         --                     

--------------------------------Alarms/Errors--------------------------------
>Port
Alarms
            Seconds   
Frequency   --        

>Ethernet
Alarms
       Seconds   
Link   2         

Errors
                Seconds   Count   Rate       
Symbol          0         0       0,00E00    
Idle            1         255     3,69E-07   
False Carrier   1         46087   1,05E-02   
FCS             0         0       0,00E00    
Jabber/Giant    0         0       0,00E00    
Runt            0         0       0,00E00    
Undersize       0         0       0,00E00    
Alignment       --        --      --         

>Upper Layer
Errors
                     Seconds   Count   Rate      
IP Header Checksum   0         0       0,00E00   
UDP Checksum         0         0       0,00E00   

--------------------------------Statistics--------------------------------
Valid Frame Counts
Total TX Frame Count   4324806   
Total RX Frame Count   4325845   

Frequency Analysis
Frequency (bps)              --    
Frequency Offset (ppm)       0     
Max. Negative Offset (ppm)   0     
Max. Positive Offset (ppm)   0     

--------------------------------System Information--------------------------------
>Module Information
Module ID:          FTB-8510B             
Revision:           1                     
Serial Number:      AZ70A3B               
Calibration Date:   2009-10-22 11:58:00   

>Software Information
Software Version:   1.13.0.27   

