EXFO Electro-Optical Engineering Inc.
Report Title: ReportTitle
Report Date: 2010-02-19 02:45:36
--------------------------------Job Information--------------------------------
Job ID:          1                            
Contractor:                                  
Customer:        Maxprogres                            
Operator Name:   Zdenek                            
Comment:         mereni propoje Boskovice --- PVT (1Gbps)  Pozn. mereno bez aktivnich prvku, switche, routery apod.   

--------------------------------Test Configuration--------------------------------
Test Name:          TEST                   
Interface Type:     Ethernet 10/100/1000   
Application Type:   RFC 2544               
Topology:           Single Port            

>Port Configuration
                     Port 1              
Transceiver Mode     Electrical          
Speed                1Gbps               
Duplex mode          Full                
Auto-Negotiation     Disabled            
VLAN                 None                
IP Source Address    192.168.1.100       
MAC Source Address   00:03:01:08:3A:AD   

>RFC 2544
Local to Remote Throughput Maximum Rate (%)   100     
Remote to Local Throughput Maximum Rate (%)   100     
Throughput Test Time                          00:01   
Back-to-Back Test Time                        00:01   
Local to Remote Frame Loss Maximum Rate (%)   100     
Remote to Local Frame Loss Maximum Rate (%)   100     
Frame Loss Test Time                          00:01   
Latency Test Time                            00:01   
Margin (%)                            0       

Latency Max rate
No information is available

>Remote Dual Test Set
No information is available

--------------------------------Test Results--------------------------------
Start Time:    2010-02-19 02:34:51   Duration   0d 00:01:42   

>RFC 2544
Verdict        Status   
Throughput     --       
Back-to-Back   --       
Frame Loss     --       
Latency        --       

>Throughput
Layer: Layer 1-2-3
Display Results: Current
Frame Size   Local to Remote (Mbps)   Remote to Local (Mbps)   
64           1000                     1000                     
128          1000                     1000                     
256          1000                     1000                     
512          1000                     1000                     
1024         --                       --                       
1280         --                       --                       
1518         --                       --                       

>Back-to-Back
Layer: Layer 1-2-3
Display Results: Current
Frame Size   Local to Remote (Frames/Burst)   Remote to Local (Frames/Burst)   
64           --                            --                            
128          --                            --                            
256          --                            --                            
512          --                            --                            
1024         --                            --                            
1280         --                            --                            
1518         --                            --                            

>Frame Loss
Display Results: Current
Displayed Step: 100
Frame Size   Local to Remote(%)   Remote to Local(%)   
64           --                   --                   
128          --                   --                   
256          --                   --                   
512          --                   --                   
1024         --                   --                   
1280         --                   --                   
1518         --                   --                   

>Latency
Display Results: Current
Latency Mode: Cut Through
Frame Size   Round Trip Time (ms)   
64           --                     
128          --                     
256          --                     
512          --                     
1024         --                     
1280         --                     
1518         --                     

--------------------------------Alarms/Errors--------------------------------
>Port
Alarms
            Seconds   
Frequency   --        

>Ethernet
Alarms
       Seconds   
Link   2         

Errors
                Seconds   Count   Rate       
Symbol          0         0       0,00E00    
Idle            1         255     2,89E-07   
False Carrier   1         42370   6,96E-03   
FCS             0         0       0,00E00    
Jabber/Giant    0         0       0,00E00    
Runt            0         0       0,00E00    
Undersize       0         0       0,00E00    
Alignment       --        --      --         

>Upper Layer
Errors
                     Seconds   Count   Rate      
IP Header Checksum   0         0       0,00E00   
UDP Checksum         0         0       0,00E00   

--------------------------------Statistics--------------------------------
Valid Frame Counts
Total TX Frame Count   6041621   
Total RX Frame Count   6042110   

Frequency Analysis
Frequency (bps)              --    
Frequency Offset (ppm)       0     
Max. Negative Offset (ppm)   0     
Max. Positive Offset (ppm)   0     

--------------------------------System Information--------------------------------
>Module Information
Module ID:          FTB-8510B             
Revision:           1                     
Serial Number:      AZ70A3B               
Calibration Date:   2009-10-22 11:58:00   

>Software Information
Software Version:   1.13.0.27   

