# Audio Filter

Applies a Low pass filter to an audio stream. Remember to Mute the audio to hear the pure filtered sound.

The low pass filter acts as a gate, only letting frequencies below the cut off value through.

The F knob controls the cut off frequency, between 0 and 22050 Hz.

The Q knob controls the resonance drive.

A low frequency cutoff and strong resonance can give an acidy or dampened underwater effect.

(Be careful! Adjust your volume! Certain knob combinations can give off loud undesired schreeching noises!)

Music: Delv-X: Megaman theme (cover)