= PicoBlaze Online
Writing 0x
 to address 0x
 of 
Address: 0x
 Content: 0x
Status: 
1000 Mb/s
 100 Mb/s
  10 Mb/s
Disconnected
Initializing peripherals... 
MAC 
HOST 
PHY 
SFP 
SMA 
PCS/PMA 
Port
... 
Wait
ERROR!
FAILED!
DONE!
88E1111 
Unsupported SFP module!
No SFP detected!