USBHost FT232 UART Echo Sample Readme
-------------------------------------

This demonstration application reads data from an FT232 device on USB port 1 and relays it to the UART interface. The FT232 and the UART are set to 9600 baud.

This sample was previously called USBHostFT232Echo.

Restrictions:
- N/A

Known bugs:
- N/A

Features requests:
- N/A
