=============================================================================
List of generated methods in project: Generator

THIS TEXT DESCRIPTION IS GENERATED BY THE TOOL. DO NOT MODIFY IT.
=============================================================================

Module "Potvrzreni_in" (bean BitIO)
   - Potvrzreni_in_GetVal -Returns the input/output value. If the direction is [input] then the input value of the pin is read 
                and returned. If the direction is [output] then the last written value is returned (see <Safe mode> property 
                for limitations). This method cannot be disabled if direction is [input].

Module "Potvrzeni_out" (bean BitIO)
   - Potvrzeni_out_GetVal -Returns the input/output value. If the direction is [input] then the input value of the pin is read 
                and returned. If the direction is [output] then the last written value is returned (see <Safe mode> property 
                for limitations). This method cannot be disabled if direction is [input].
   - Potvrzeni_out_PutVal -The specified output value is set. If the direction is [input], the component saves the value to a 
                memory or a register and this value will be written to the pin after switching to the output mode (using 
                [SetDir(TRUE)]; see <Safe mode> property for limitations). If the direction is [output], it writes the value to 
                the pin. (Method is available only if the direction = _[output]_ or _[input/output]_).
   - Potvrzeni_out_ClrVal -Clears (set to zero) the output value. It is equivalent to the [PutVal(FALSE)]. This method is 
                available only if the direction = _[output]_ or _[input/output]_.
   - Potvrzeni_out_SetVal -Sets (to one) the output value. It is equivalent to the [PutVal(TRUE)]. This method is available 
                only if the direction = _[output]_ or _[input/output]_.

Module "Vystupni_port" (bean ByteIO)
   - Vystupni_port_GetDir -Returns selected direction.
   - Vystupni_port_GetVal -Returns the value of the Input/Output component. If the direction is [input] then it reads the input 
                value of the pins and returns it. If the direction is [output] then it returns the last written value (see 
                <Safe mode> property for limitations).
   - Vystupni_port_PutVal -Specified value is passed to the Input/Output component. If the direction is [input] saves the value 
                to a memory or a register, this value will be written to the pins after switching to the output mode - using 
                [SetDir(TRUE)] (see <Safe mode> property for limitations). If the direction is [output] it writes the value to 
                the port. (Method is available only if the Direction = _[output]_ or _[input/output]_).
   - Vystupni_port_GetBit -Returns the value of the specified bit/pin of the Input/Output component. If the direction is 
                [input] then it reads the input value of the pin and returns it. If the direction is [output] then it returns 
                the last written value (see <Safe mode> property for limitations).
   - Vystupni_port_PutBit -Specified value is passed to the specified bit/pin of the Input/Output component. If the direction 
                is [input] it saves the value to a memory or a register, this value will be written to the pin after switching 
                to the output mode - using [SetDir(TRUE)] (see <Safe mode> property for limitations). If the direction is 
                [output] it writes the value to the pin. (Method is available only if the Direction = _[output]_ or 
                _[input/output]_).
   - Vystupni_port_SetBit -Sets (to one) the specified bit of the Input/Output component. It is the same as [PutBit(Bit, TRUE)].
                (Method is available only if the Direction = _[output]_ or _[input/output]_).
   - Vystupni_port_ClrBit -Clears (set to zero) the specified bit of the Input/Output component. It is the same as [PutBit(Bit, 
                FALSE)]. (Method is available only if the Direction = _[output]_ or _[input/output]_).
   - Vystupni_port_NegBit -Negates (inverts) the specified bit of the Input/Output component. It is the same as [PutBit(Bit,!
                GetBit(Bit))]. (Method is available only if the Direction = _[output]_ or _[input/output]_).

Module "Frekvence_filtr" (bean TimerOut)
   - Frekvence_filtr_Enable -This method enables the component - It starts the signal generation. Events may be generated 
                (<DisableEvent>/<EnableEvent>).
   - Frekvence_filtr_Disable -This method disables the timer - it stops signal generation and events calling. When the timer is 
                disabled, it is possible to call methods <ClrValue> and <SetValue>.
   - Frekvence_filtr_SetPeriodReal -This method sets the new pulse width of the output signal. The pulse width is expressed in 
                [seconds] as a real number. To use this method the compiler have to support floating point operations.   This 
                method is available only if the runtime setting type 'from interval' is selected in the <Timing dialog box> in 
                the Runtime setting area.

Module "DAC_ILE"   (bean BitIO)
   - DAC_ILE_GetVal -Returns the input/output value. If the direction is [input] then the input value of the pin is read and 
                returned. If the direction is [output] then the last written value is returned (see <Safe mode> property for 
                limitations). This method cannot be disabled if direction is [input].
   - DAC_ILE_PutVal -The specified output value is set. If the direction is [input], the component saves the value to a memory 
                or a register and this value will be written to the pin after switching to the output mode (using 
                [SetDir(TRUE)]; see <Safe mode> property for limitations). If the direction is [output], it writes the value to 
                the pin. (Method is available only if the direction = _[output]_ or _[input/output]_).
   - DAC_ILE_ClrVal -Clears (set to zero) the output value. It is equivalent to the [PutVal(FALSE)]. This method is available 
                only if the direction = _[output]_ or _[input/output]_.
   - DAC_ILE_SetVal -Sets (to one) the output value. It is equivalent to the [PutVal(TRUE)]. This method is available only if 
                the direction = _[output]_ or _[input/output]_.

Module "EI2C2"     (bean SW_I2C)
   - EI2C2_Enable -This method enables the I2C interface for send and receive operations. This method cannot be disabled if the 
                <Enabled in init. code> property value is "no".
   - EI2C2_Disable -This method disables the I2C interface for send and receive operations.
   - EI2C2_EnableEvent -This method enables the events. This method is available only if at least one event is enabled.
   - EI2C2_DisableEvent -This method disables the events. This method is available only if at least one event is enabled.
   - EI2C2_SendChar -When working as a MASTER, this method writes 7 bits of slave address plus R/W bit = 0 to the I2C bus and 
                then writes one character (byte) to the bus. The slave address must be specified before by the "SelectSlave" 
                method or in the component initialization section of <Slave address init> property. When working as the SLAVE, 
                this method writes one character (byte) to the bus. If the ERR_NOTAVAIL error code returned, the char is 
                successfully sent to master but the master device responds by an acknowledgement instead of no acknowledgement 
                at the end of transfer. <OnError> event is called in this case.
   - EI2C2_RecvChar -When working as a MASTER, this method writes 7 bits of slave address plus R/W bit = 1 to the I2C bus and 
                then reads one character (byte) from the bus. The slave address must be specified before by the "SelectSlave" 
                method or in the component initialization section of <Slave address init> property. When working as a SLAVE, 
                this method reads one character (byte) from the bus.
   - EI2C2_SendBlock -When working as a MASTER, this method writes 7 bits of slave address plus R/W bit = 0 to the I2C bus and 
                then writes the block of characters to the bus. If the component is disabled (by the "Disable" method or 
                initialization), the block is moved to the output buffer if the <Output buffer size> property is different from 
                zero. The content of the output buffer is sent immediately with the stop condition at the end when the 
                component is enabled by the "Enable" method. After the output buffer transmission, the whole output buffer is 
                cleared. The slave address must be specified before by the "SelectSlave" method or in component initialization 
                section of <Slave address init> property. When working as a SLAVE, this method writes block of characters to 
                the bus. If the ERR_NOTAVAIL error code is returned, the whole block is successfully sent to a master but the 
                master device responds by an acknowledgement instead of no acknowledgment sent at the end of the last block 
                byte transfer. <OnError> event is called in this case.
   - EI2C2_RecvBlock -When working as a MASTER, this method writes 7 bits of slave address plus R/W bit = 1 to the I2C bus and 
                then reads the block of characters from the bus. The slave address must be specified before by the 
                "SelectSlave" method or in component initialization section of <Slave address init> property. When working as a 
                SLAVE, this method reads the block of characters from the bus.
   - EI2C2_SendStop -When working as a MASTER, if the <Automatic stop condition> property value is 'no', this method sends a 
                valid stop condition to the serial data line of the I2C bus to terminate the communication on the bus after 
                using send methods. This method is enabled only if the component is in MASTER mode and <Automatic stop 
                condition> property value is 'no'
   - EI2C2_SelectSlave -When working as a MASTER, this method selects a new slave for communication by its slave address value. 
                Any send or receive method are directed to or from the selected device, until a new slave device is selected by 
                this method. If the selected slave uses 10-bit slave addressing, as the parameter 7 bits must be passed, which 
                involves 10-bit addressing (11110XX), including two MSBs of slave address (XX). The second byte of the 10-bit 
                slave address must be sent to the slave as a general character of send methods. This method is available only 
                if the component is in MASTER mode.
   - EI2C2_GetSelected -When working as a MASTER, this method returns the identification address value of the slave, which is 
                currently selected for communication with the master. If the current slave uses 10-bit slave addressing, the 
                method returns the first 7 bits only, which involves 10-bit addressing (11110XX), including two MSBs of the 
                slave address (XX). This method is not able to return the rest value of 10-bit slave address. This method is 
                available only if the component is in MASTER mode.

Module "Cpu"       (bean MC9S08GT16A_44)
   - Cpu_EnableInt -Enables maskable interrupts
   - Cpu_DisableInt -Disables maskable interrupts
   - Cpu_Delay100US -This method realizes software delay. The length of delay is at least 100 microsecond multiply input 
                parameter [us100]. As the delay implementation is not based on real clock, the delay time may be increased by 
                interrupt service routines processed during the delay. The method is independent on selected speed mode.

===================================================================================
