A B C D E F G H I K L M N O P R S T U V W Z

## D

data - Variable in class fields.DataRecord
dataBits - Static variable in class core.IqrfDeviceModel
DataField - Class in fields
  Model for the WM-Bus Data-Field.
DataField() - Constructor for class fields.DataField
DataFieldCode - Enum in enumerations
  Data-field codes specified in Wireless M-Bus, their binary representations, meanings and sizes of described data.
DataFieldCode(String, int, String) - Constructor for enum enumerations.DataFieldCode
dataFieldCode - Variable in class fields.DataRecord.DIF
dataHeader - Variable in class fields.DataField
DataHeader - Class in fields
  Model for the WM-Bus Data-Field header.
DataHeader() - Constructor for class fields.DataHeader
DataHeaderType - Enum in enumerations
  Data header types supported by Wireless M-Bus.
DataHeaderType(int, String) - Constructor for enum enumerations.DataHeaderType
DataRecord - Class in fields
  Model for the WM-Bus Data record Keeps one DIF, one VIF, a list of DIFEs, a list of VIFEs and a list of Bytes for data (payload).
DataRecord() - Constructor for class fields.DataRecord
DataRecord.DataRecordHeaderBase - Class in fields
  Base for DIFs, VIFs, DIFEs and VIFEs.
DataRecord.DIF - Class in fields
  Model for the WM-Bus DIF.
DataRecord.DIFE - Class in fields
  Model for the WM-Bus DIFE.
DataRecord.VIF - Class in fields
  Model for the WM-Bus VIF.
DataRecord.VIFE - Class in fields
  Model for the WM-Bus VIFE.
DataRecordDialogController - Class in ui
  Layer 3 controller
DataRecordDialogController() - Constructor for class ui.DataRecordDialogController
DataRecordHeaderBase() - Constructor for class fields.DataRecord.DataRecordHeaderBase
DataRecordHeaderBase(boolean) - Constructor for class fields.DataRecord.DataRecordHeaderBase
dataRecords - Variable in class fields.DataField
dataRecords - Variable in class ui.FrameDialogController
decrypt(EncryptionMethod, byte[], byte[]) - Static method in class core.Crypter
  Decrypts given message by given encryption method with given key.
decrypt(EncryptionMethod, byte[], byte[], byte[]) - Static method in class core.Crypter
  Decrypts given message by given encryption method, with given key, using given initialization vector (can be null).
DEFAULT_COMM_PORT - Static variable in class senders.CommSender
DEFAULT_DST_IP - Static variable in class senders.UdpSender
DEFAULT_DST_PORT - Static variable in class senders.UdpSender
DEFAULT_INTERVAL_SECONDS - Static variable in class senders.UdpSender
DEFAULT_SRC_IP - Static variable in class senders.UdpSender
DEFAULT_SRC_PORT - Static variable in class senders.UdpSender
des(int, byte[], byte[], byte[]) - Static method in class core.Crypter
device - Variable in class senders.CommSender
deviceSubunitBit - Variable in class fields.DataRecord.DIFE
deviceType - Variable in class core.IqrfDeviceModel
DeviceType - Enum in enumerations
  Device Types specified in Wireless M-Bus, their hexadecimal representations and meanings.
DeviceType(int, String) - Constructor for enum enumerations.DeviceType
deviceType - Variable in class fields.AField
deviceType - Variable in class fields.DataHeader
dif - Variable in class fields.DataRecord
DIF() - Constructor for class fields.DataRecord.DIF
DIF(boolean, boolean, String, String) - Constructor for class fields.DataRecord.DIF
DIFE() - Constructor for class fields.DataRecord.DIFE
DIFE(Byte) - Constructor for class fields.DataRecord.DIFE
DIFE(boolean, boolean, String, String) - Constructor for class fields.DataRecord.DIFE
difeChbs - Variable in class ui.DataRecordDialogController
difes - Variable in class fields.DataRecord
disablePortScanning(boolean) - Method in class ui.InitialWindowController
  Disables/enables controls to start port scanning.
disableSenderProperties(boolean) - Method in class ui.InitialWindowController
  Disables/enables controls to change connection properties.
disableSenderSwitching(boolean) - Method in class ui.InitialWindowController
  Disables/enables controls to change connection switching.
dr - Variable in class ui.DataRecordDialogController
drdc - Variable in class ui.FrameDialogController
dstIP - Variable in class senders.UdpSender
dstPort - Variable in class senders.UdpSender

A B C D E F G H I K L M N O P R S T U V W Z