A B C D E F G H I K L M N O P R S T U V W Z

## S

saveDataRecordParameters() - Method in class ui.DataRecordDialogController
  Takes inputs from the GUI and stores them in the underlying data record object.
saveFrameParameters() - Method in class ui.FrameDialogController
  Takes inputs from the GUI and stores them in the underlying frame object.
scanForPorts() - Method in class core.IqrfDeviceModel
  Scans for open serial ports.
scheduler - Variable in class senders.Sender
scheduler - Variable in class senders.UdpSender
seconds - Variable in enum senders.Sender.SendingInterval
Sender - Class in senders
Sender() - Constructor for class senders.Sender
sender - Variable in class ui.InitialWindowController
sender - Variable in class ui.NonInteractiveCLI
Sender.SendingInterval - Enum in senders
  Supported sending intervals.
senders - package senders
SendingInterval(int, String) - Constructor for enum senders.Sender.SendingInterval
serial - Variable in class core.IqrfDeviceModel
serial - Variable in class fields.AField
serial - Variable in class fields.DataHeader
serialPort - Variable in class core.IqrfDeviceModel
setAccessNumber(Byte) - Method in class fields.DataHeader
setAccessNumber(String) - Method in class fields.DataHeader
setAField(AField) - Method in class core.Frame
setByDataRecord(DataRecord) - Method in class ui.DataRecordDialogController
  Sets this window controls by given DataRecord
setByDIFE(Byte) - Method in class ui.DataRecordDialogController
  Sets the DIFE section by a DIFE byte.
setByFrame(Frame) - Method in class core.IqrfDeviceModel
  Sets the device configuration to match given frame parameter's.
setByFrame(Frame) - Method in class ui.FrameDialogController
  Sets this window controls by given Frame
setByVIFE(Byte) - Method in class ui.DataRecordDialogController
  Sets the VIFE section by a VIFE byte.
setCField(CField) - Method in class core.Frame
setCIField(CIField) - Method in class core.Frame
setControl(Byte) - Method in class fields.CField
setControl(CCode) - Method in class fields.CField
setControl(CICode) - Method in class fields.CIField
setControl(Byte) - Method in class fields.CIField
setData(Byte[]) - Method in class fields.DataRecord
setDataField(DataField) - Method in class core.Frame
setDataFieldCode(DataFieldCode) - Method in class fields.DataRecord.DIF
setDataFieldCode(String) - Method in class fields.DataRecord.DIF
setDataHeader(DataHeader) - Method in class fields.DataField
setDeviceSubunitBit(boolean) - Method in class fields.DataRecord.DIFE
setDeviceType(Byte) - Method in class fields.AField
setDeviceType(DeviceType) - Method in class fields.AField
setDeviceType(Byte) - Method in class fields.DataHeader
setDIF(DataRecord.DIF) - Method in class fields.DataRecord
setEnabled(boolean) - Method in class core.PeriodicTelegramBase
setEncryptionIV(String) - Method in class fields.DataField
setEncryptionKey(String) - Method in class fields.DataField
setEncryptionMethod(EncryptionMethod) - Method in class fields.DataField
setExtensionBit(boolean) - Method in class fields.DataRecord.DataRecordHeaderBase
setFluctuated(boolean) - Method in class ui.InitialWindowController.GUIPeriodicTelegram
setFrame(Frame) - Method in class core.PeriodicTelegramBase
setFunctionCode(FunctionCode) - Method in class fields.DataRecord.DIF
setFunctionCode(String) - Method in class fields.DataRecord.DIF
setHeaderType(DataHeaderType) - Method in class fields.DataHeader
setIndex(ScheduledFuture<?>) - Method in class core.PeriodicTelegramBase
setInterval(Sender.SendingInterval) - Method in class core.PeriodicTelegramBase
setManId(Byte[]) - Method in class fields.DataHeader
setManID(Byte[]) - Method in class fields.MField
setManID(String) - Method in class fields.MField
setMField(MField) - Method in class core.Frame
setMode(Mode) - Method in class core.Frame
setMultiplier(Integer) - Method in class fields.DataRecord.VIF
setPostamble(Ambles.Postamble) - Method in class core.Frame
setPreamble(Ambles.Preamble) - Method in class core.Frame
setSerial(String) - Method in class fields.AField
setSerial(Byte[]) - Method in class fields.DataHeader
setSignature(Byte[]) - Method in class fields.DataHeader
setSpecialCode(String) - Method in class fields.DataRecord.VIFE
setStatus(Boolean) - Method in class core.PeriodicTelegramBase
setStatus(Boolean) - Method in class ui.InitialWindowController.GUIPeriodicTelegram
setStatusCodes(Byte) - Method in class fields.DataHeader
setStatusCodes(String) - Method in class fields.DataHeader
setStorageNumberBit(boolean) - Method in class fields.DataRecord.DIF
setStorageNumberBits(String) - Method in class fields.DataRecord.DIFE
setTariffBits(String) - Method in class fields.DataRecord.DIFE
setValueType(String) - Method in class fields.DataRecord.VIF
setValueType(ValueType) - Method in class fields.DataRecord.VIF
setVerification(Byte[]) - Method in class fields.DataField
setVerification(Byte[]) - Method in class fields.DataHeader
setVersion(String) - Method in class fields.AField
setVersion(Byte) - Method in class fields.DataHeader
setVIF(DataRecord.VIF) - Method in class fields.DataRecord
shutdown() - Method in class core.IqrfDeviceModel
  Terminates the connection and releases the serial port.
shutdown() - Method in class senders.CommSender
shutdown() - Method in class senders.Sender
  Terminates the sending process and, if applicable, connected devices and channels.
signature - Variable in class fields.DataHeader
sleep() - Method in class core.IqrfDeviceModel
  Triggers sleep mode on the device, if it is awake.
SleepMode(String, String) - Constructor for enum core.IqrfDeviceModel.SleepMode
specialCode - Variable in class fields.DataRecord.VIFE
srcIP - Variable in class senders.UdpSender
srcPort - Variable in class senders.UdpSender
stackConnection - Variable in class ui.InitialWindowController
start(Stage) - Method in class core.GUI
status - Variable in class core.PeriodicTelegramBase
statusByte - Variable in class core.IqrfDeviceModel
statusChbs - Variable in class ui.FrameDialogController
statusCheckBoxesChanged(ActionEvent) - Method in class ui.FrameDialogController
  Sets the Status bits text by the status byte checkboxes.
StatusCode - Enum in enumerations
  Status codes specified in Wireless M-Bus, their meanings bit order.
StatusCode(String, int) - Constructor for enum enumerations.StatusCode
statusCodes - Variable in class fields.DataHeader
stopBits - Static variable in class core.IqrfDeviceModel
storageNumberBit - Variable in class fields.DataRecord.DIF
storageNumberBits - Variable in class fields.DataRecord.DIFE
supportedValues() - Static method in enum enumerations.Mode
swapConnectionPane() - Method in class ui.InitialWindowController
  Cycles the connection panes in the stack pane like a card deck.

A B C D E F G H I K L M N O P R S T U V W Z