A B C D E F G H I K L M N O P R S T U V W Z

## C

calculatePreamble(int, String) - Static method in class fields.Ambles
  Concatenates preamble bits from n times "01" and an appendix
cancel(ScheduledFuture<?>) - Method in class senders.Sender
  Removes given scheduler ID from the periodic sending process.
cancelAllTelegrams() - Method in class ui.InitialWindowController
  Disables the sending of all defined telegrams.
cbEncryptionChanged() - Method in class ui.FrameDialogController
  Updates controls to match selected encryption type.
cbValueTypeChanged() - Method in class ui.DataRecordDialogController
CCode - Enum in enumerations
  C-Field codes specified in Wireless M-Bus, their meanings and hexadecimal representations.
CCode(int, String) - Constructor for enum enumerations.CCode
CField - Class in fields
  Model for the WM-Bus C-Field
CField() - Constructor for class fields.CField
CField(CCode) - Constructor for class fields.CField
CField(byte) - Constructor for class fields.CField
changed(ObservableValue<? extends Boolean>, Boolean, Boolean) - Method in class ui.ValidatedChangeListener
  Validates the field and raises an alert warning dialog in case of failure.
chbAnyAppError - Variable in class ui.FrameDialogController
chbAppBusy - Variable in class ui.FrameDialogController
chbDIFEbit1 - Variable in class ui.DataRecordDialogController
chbDIFEbit2 - Variable in class ui.DataRecordDialogController
chbDIFEbit3 - Variable in class ui.DataRecordDialogController
chbDIFEbit4 - Variable in class ui.DataRecordDialogController
chbDIFEbit5 - Variable in class ui.DataRecordDialogController
chbDIFEbit6 - Variable in class ui.DataRecordDialogController
chbDIFEbit7 - Variable in class ui.DataRecordDialogController
chbDIFEbit8 - Variable in class ui.DataRecordDialogController
chbDifExtensionBit - Variable in class ui.DataRecordDialogController
chbNoError - Variable in class ui.FrameDialogController
chbPermanentError - Variable in class ui.FrameDialogController
chbPowerLow - Variable in class ui.FrameDialogController
chbStatusBitManSpecific5 - Variable in class ui.FrameDialogController
chbStatusBitManSpecific6 - Variable in class ui.FrameDialogController
chbStatusBitManSpecific7 - Variable in class ui.FrameDialogController
chbStorageNumberBit - Variable in class ui.DataRecordDialogController
chbTempError - Variable in class ui.FrameDialogController
chbVIFEbit1 - Variable in class ui.DataRecordDialogController
chbVIFEbit2 - Variable in class ui.DataRecordDialogController
chbVIFEbit3 - Variable in class ui.DataRecordDialogController
chbVIFEbit4 - Variable in class ui.DataRecordDialogController
chbVIFEbit5 - Variable in class ui.DataRecordDialogController
chbVIFEbit6 - Variable in class ui.DataRecordDialogController
chbVIFEbit7 - Variable in class ui.DataRecordDialogController
chbVIFEbit8 - Variable in class ui.DataRecordDialogController
chbVifExtensionBit - Variable in class ui.DataRecordDialogController
checkCRC(Byte[]) - Static method in class fields.CRCField
  Validates given Byte[ ] against its CRC-DNP, which has to the last two Bytes in the Byte[ ].
CICode - Enum in enumerations
  CI-Field codes specified in Wireless M-Bus, their meanings and hexadecimal representations.
CICode(int, String) - Constructor for enum enumerations.CICode
CIField - Class in fields
  Model for the WM-Bus CI-Field
CIField(CICode) - Constructor for class fields.CIField
CIField(byte) - Constructor for class fields.CIField
CIField() - Constructor for class fields.CIField
CLI - Class in core
  Manages the app, when started from CLI.
CLI() - Constructor for class core.CLI
CLI.CLIPeriodicTelegram - Class in core
  Frame object extended with periodicity properties and scheduler indices.
CLIPeriodicTelegram(Frame) - Constructor for class core.CLI.CLIPeriodicTelegram
closeStage() - Method in class ui.DataRecordDialogController
closeStage() - Method in class ui.FrameDialogController
cmbCCode - Variable in class ui.FrameDialogController
cmbCICode - Variable in class ui.FrameDialogController
cmbDataFieldCode - Variable in class ui.DataRecordDialogController
cmbDeviceType - Variable in class ui.FrameDialogController
cmbDHType - Variable in class ui.FrameDialogController
cmbEncryption - Variable in class ui.FrameDialogController
cmbFunctionField - Variable in class ui.DataRecordDialogController
cmbMode - Variable in class ui.FrameDialogController
cmbMultiplier - Variable in class ui.DataRecordDialogController
cmbValueType - Variable in class ui.DataRecordDialogController
Coder - Class in core
  Encodes WM-Bus types.
Coder() - Constructor for class core.Coder
codeTypeF(Calendar, boolean, boolean) - Static method in class core.Coder
  Encodes a time instant into Wireless M-Bus Type F structured Byte[ ].
codeTypeG(Calendar) - Static method in class core.Coder
  Encodes a time instant into Wireless M-Bus Type G structured Byte[ ].
colEnabled - Variable in class ui.InitialWindowController
colFluctuation - Variable in class ui.InitialWindowController
colFrame - Variable in class ui.InitialWindowController
colInterval - Variable in class ui.InitialWindowController
colStatus - Variable in class ui.InitialWindowController
comboBoxCICodeChanged() - Method in class ui.FrameDialogController
  Sets the Header drop down menu to match the CI one.
comboBoxDataHeaderTypeChanged() - Method in class ui.FrameDialogController
  Sets the CI-code drop down menu to match the Header type one.
commPortName - Variable in class senders.CommSender
CommSender - Class in senders
  Manages periodic sending of frames over a serial port via IQRF device.
CommSender(String) - Constructor for class senders.CommSender
confirmed - Variable in class ui.DataRecordDialogController
confirmed - Variable in class ui.FrameDialogController
connect(String) - Method in class core.IqrfDeviceModel
  Attempts to connect to the IQRF module on the given serial port.
connect() - Method in class senders.CommSender
  Creates an IQRF device model for the device on port specified in this sender.
connect() - Method in class senders.Sender
  Initiates connection with the output channel.
connected - Variable in class senders.Sender
connectionGroup - Variable in class ui.InitialWindowController
construct() - Method in class core.Frame
  Calculates all available fields and calls getBytes() on them.
construct() - Method in class core.FrameA
construct() - Method in class core.FrameB
control - Variable in class fields.CField
control - Variable in class fields.CIField
core - package core
crc - Variable in class fields.CRCField
CRC_TABLE - Static variable in class fields.CRCField
CRCField - Class in fields
  Model for the WM-Bus CRC-Fields
CRCField(Byte[]) - Constructor for class fields.CRCField
CRCField(List<Byte>) - Constructor for class fields.CRCField
Crypter - Class in core
  Encrypts and decrypts byte arrays, using encryption techniques found in Wireless M-bus.
Crypter() - Constructor for class core.Crypter

A B C D E F G H I K L M N O P R S T U V W Z