A B C D E F G H I K L M N O P R S T U V W Z

## M

main(String[]) - Static method in class core.CLI
  Starts either GUI, interactive CLI, machine CLI, or prints help if none was specified.
main(String[]) - Static method in class core.GUI
main(String[]) - Static method in class core.IqrfDeviceModel
makeAddress() - Method in class core.IqrfDeviceModel
makeCRC(Byte[]) - Static method in class fields.CRCField
  Calculates CRC-DNP of given bytes.
manID - Variable in class core.IqrfDeviceModel
manId - Variable in class fields.DataHeader
manID - Variable in class fields.MField
manIdToHex(String) - Static method in class fields.MField
  Converts given manufacturer ID or manufacturer 3-letter code to bytes by the algorithm specified in Wireless M-Bus.
manufacturer - Variable in class fields.MField
messageTerminator - Static variable in class core.IqrfDeviceModel
MField - Class in fields
  Model for the WM-Bus M-Field
MField(String) - Constructor for class fields.MField
MField(Byte[]) - Constructor for class fields.MField
MField() - Constructor for class fields.MField
mirrorBytes(Byte[]) - Static method in class core.ByteUtils
  Mirrors a Byte[ ], so that the first element is last and the last is first.
mode - Variable in class core.Frame
mode - Variable in class core.IqrfDeviceModel
Mode - Enum in enumerations
  Wireless M-Bus physical layer modes, their names, encodings they use and their IQRF numbering.
Mode(String, Encoding, int) - Constructor for enum enumerations.Mode
multiplier - Variable in class fields.DataRecord.VIF

A B C D E F G H I K L M N O P R S T U V W Z