On/Off controller
On/Off controller (Schmidt's trigger)
Library
GFLIB
Description
Switches the output between two states (On/Off) according to the input error.
Parameters and dialog box
The On/Off controller block dialog box appears as follows:
If the input error is greater than thresh, On value is assigned to the output.If the input error is lower than thresh, Off value is assigned to the output.
Inputs and outputs
Inputs:
in - input error
Outputs:
out - output signal
See also
Continuous PID, Discrete PID