3-PH ADC
3-phase A/D converter
Library
GMCLIB
Description
Performs an 3-phase A/D converter with user-defined resolution, input range and sampling period.
Parameters and dialog box
The ADC block dialog box appears as follows:
The block constrains the 3-phase input signal to n-bit resolution. The entered range is divided into 2^n equal levels. The input is converted at the beginning of sampling period Ts and the output holds its value for the rest the period. Simply the block packs 3 ADC into one block.
Inputs and outputs
Inputs:
in - 3-phase input signal
Outputs:
out - 3-phase output signal
See also
ADC