Clark
Clark's transformation
Library
GMCLIB
Description
Performs a Clark's transformation on to 3-phase input signal according to the following equations:
Sum of the input signals has to be zero at each time sample. If this assumption is violated, the previous equations don't hold anymore.
Inputs and outputs
Inputs:
a,b,c - 3-phase input signal in stationary frame
Outputs:
alpha, beta - 2-phase output signal in stationary frame
See also
ClarkeInv, ClarkeUnbalanced, ClarkeInvUnbalanced, Park, ParkInv,