Vector Limit
Limits amplitude of the input vector.
Library
GFLIB
Description
Limits amplitude of the input vector and returns its d-q coordinates.
Parameters and dialog box
The Vector Limit block dialog box appears as follows:
Inputs are components of the input vector in d-q coordinate system. The amplitude is limited to maximum value specified in Amplitude limit parameter. The function returns d-q output vector components.
Inputs and outputs
Inputs:
d_in - d-axis component of the input signal
q_in - q-axis component of the input signal
Outputs:
d_out - d-axis component of the output signal
q_out - q-axis component of the output signal
Flag - indicates limitation (1=limited, 0=remains)